**
**   Restart SSD SP analysis with eigensolution by Lanczos
**
*HEADING
 Restart SSD SP analysis using Lanczos eigensolution
**
*RESTART, READ, STEP=1, END STEP
***-------------------------------------------------------------------------
** step 2 - Subspace-based SSD
***-------------------------------------------------------------------------
*STEP
 Subspace-based SSD
*STEADY STATE DYNAMICS, SUBSPACE PROJECTION=CONSTANT, INTERVAL=RANGE, FREQUENCY SCALE=LINEAR
1, 150, 150
*SELECT EIGENMODES, GENERATE
*CLOAD
mnt2, 3, 1.0
mnt7, 3, -1.0
*OUTPUT, HISTORY
*NODE OUTPUT,NSET=output
U, V, A
*PRINT, SOLVE=YES
*END STEP