*HEADING
 3D SLUMP TEST, LINEAR DRUCKER PRAGER (MISES)
 (ANG FRIC=0.0);  BETA=0.00; d=2.0E-3
 CCL12 ELEMENTS
 Uses 2D dependency file  concreteslump_beta0
*SYMMETRIC MODEL GENERATION,REVOLVE,NODEOFF=500,ELEMENT=500
 180.0, 2, , C
*NSET,NSET=SECT,GEN
*ELSET,ELSET=SECT,GEN
*NSET,NSET=PLANE,GEN
*BOUNDARY
 CENT,1
 BOT,2
 PLANE, 3
*STEP,INC=100,NLGEOM
 DIMENSIONLESS SLUMP TEST UNDER GRAVITY LOAD
*STATIC
.2,1.00
*DLOAD
ALLE,GRAV,.66666,  0.0,-1.0,0.0
*EL PRINT,FREQUENCY=0
*NODE PRINT,FREQUENCY=0
*MONITOR, NODE=101, DOF=2
*OUTPUT,FIELD
*NODE OUTPUT,NSET=ALLN
U,
*ELEMENT OUTPUT
S, PE, PEEQ
*END STEP