*HEADING
: PATCH TEST FOR BEAM ELEMENTS  [B22]
*ELEMENT,TYPE=B22
*INCLUDE,INPUT=ebmod1p6.inp
*STEP,PERTURBATION
*STATIC
*BOUNDARY
 END1,1,,0.01
 END1,2
 END2,1,,0.11
 END2,2
*INCLUDE,INPUT=ebmod2p6.inp
*END STEP
*STEP,NLGEOM
*STATIC
*CLOAD
207, 1, 3000.
*BOUNDARY
END1,1,6
END2,2
*EL PRINT,SUMMARY=NO,ELSET=EL2
S,E
*OUTPUT,FIELD
*ELEMENT OUTPUT,ELSET=EL2
S,E
*NODE OUTPUT
U,RF
*NODE PRINT,SUMMARY=NO
U,RF
*END STEP
*STEP,PERTURBATION
*STATIC
*BOUNDARY
 END1,1,,0.01
 END1,2
 END2,1,,0.11
 END2,2
*INCLUDE,INPUT=ebmod2p6.inp
*END STEP