*HEADING
EB2IEXD1: DLOADS AND *TEMPERATURE FOR STRESS-DISPLACEMENT ELEMENTS  [B22H]
*NODE,NSET=ALL
*ELEMENT,TYPE=B22H, ELSET=EALL
*BEAM GENERAL SECTION,SECTION=BOX,DENSITY=0.16667, ELSET=EALL
2., 3., .01, .02, .01, .02
0.,  0., -1.
3.E6,1.1538E6, .0001
*INITIAL CONDITIONS,TYPE=TEMPERATURE
 ALL, -10., 0.
*BOUNDARY
ALL,1,2
ALL,6
*STEP,PERTURBATION
*STATIC
*DLOAD
 1, CENT, 3000., 7.5, 0., 0.,  0., 0., 1.
*EL PRINT
 LOADS,
*NODE PRINT
 RF,
*END STEP
*STEP,PERTURBATION
*STATIC
*DLOAD
1,CENTRIF,129310.32,7.5,0.,0.,0.,0.,1.
*END STEP
*STEP,PERTURBATION
*STATIC
*DLOAD
 1, GRAV, 1000., 1., 0., 0.
*END STEP
*STEP,PERTURBATION
*STATIC
*DLOAD
 1, PX, 1000.
*END STEP
*STEP,PERTURBATION
*STATIC
*DLOAD
 1, PY, 2000.
*END STEP
*STEP,PERTURBATION
*STATIC
*DLOAD
 1, P2, 2000.
*END STEP
*STEP
*STATIC
*TEMPERATURE,OP=NEW
 ALL, 20., 6.71141
*EL PRINT
 SF,
*NODE PRINT
 RF,
*END STEP
*STEP
*STATIC
*BOUNDARY,OP=NEW
1,1,2
1,6
*TEMPERATURE,OP=MOD
*EL PRINT,FREQ=0
*NODE PRINT
 U,
*END STEP