*HEADING
EB32GISD: BEAM GENERAL SECTION, SECTION=GENERAL (I)  [B31]
*NODE
*NGEN,NSET=ALL
*ELEMENT,TYPE=B31, ELSET=EALL
*ELSET, ELSET=FOUR
*BEAM GENERAL SECTION,SECTION=GENERAL, ELSET=EALL
1.4, 1.312095, 0.0, .5846667, .01866
0., 0., -1.
3.E6, 1.1538E6, .001
*CENTROID
*SHEAR CENTER
*BOUNDARY
1, 1, 6
*STEP,PERTURBATION
*STATIC
*CLOAD
11,2,25.
*EL PRINT
SF,
*NODE PRINT
 U,COORD
*END STEP
*STEP,PERTURBATION
*STATIC
*CLOAD
11,4,25.
*END STEP