*HEADING
: DLOADS AND *TEMPERATURE FOR STRESS-DISPLACEMENT ELEMENTS  [B32OSH]
*NODE,NSET=ALL
*ELEMENT,TYPE=B32OSH, ELSET=EALL
*BEAM GENERAL SECTION,SECTION=I,DENSITY=0.16667, ELSET=EALL
1.2, 2.4, 3., 2., .02, .02, .02
0. ,  0., -1.
3.E6, 1.1538E6, .0001
*INITIAL CONDITIONS,TYPE=TEMPERATURE
 ALL, -10., 0.
*BOUNDARY
ALL,1,7
*STEP,PERTURBATION
*STATIC
*DLOAD
 1, CENT, 3000., 7.5, 0., 0.,  0., 0., 1.
*EL PRINT
 LOADS,
*NODE PRINT
 RF,
*END STEP
*STEP,PERTURBATION
*STATIC
*DLOAD
1,CENTRIF,122282.36,7.5,0.,0.,0.,0.,1.
*END STEP
*STEP,PERTURBATION
*STATIC
*DLOAD
 1, GRAV, 1000., 1., 0., 0.
*END STEP
*STEP,PERTURBATION
*STATIC
*DLOAD
 1, PX, 1000.
*END STEP
*STEP,PERTURBATION
*STATIC
*DLOAD
 1, PY, 2000.
*END STEP
*STEP,PERTURBATION
*STATIC
*DLOAD
 1, PZ, 1000.
*END STEP
*STEP,PERTURBATION
*STATIC
*DLOAD
 1, P1, 1000.
*END STEP
*STEP,PERTURBATION
*STATIC
*DLOAD
 1, P2, 2000.
*END STEP
*STEP
*STATIC
*TEMPERATURE,OP=NEW
 ALL, 20., 8.4033613
*EL PRINT
 SF,
*NODE PRINT
 RF,
*END STEP
*STEP
*STATIC
*BOUNDARY,OP=NEW
1,1,7
*TEMPERATURE,OP=MOD
*EL PRINT,FREQ=0
*NODE PRINT
 U,
*END STEP