*HEADING
: SIMPLE CONTACT TEST; SMALL SLIDING [CPE8,R2D2]
********************
** Features Tested:
** *IMPORT
********************
*IMPORT,STEP=2, STATE=YES, UPDATE=NO
DBODY,RBODY
*BOUNDARY
999,1,2
999,6,6
DTOP,2,2
********************
**
** STEP 3: ADD FRICTION
**
*STEP,NLGEOM
*STATIC
1.,1.
*CHANGE FRICTION,INTERACTION=RDINT
*FRICTION
0.3,
*END STEP
********************
********************
**
** STEP 4: SLIDE WITH FRICTION
**
*STEP,NLGEOM
*STATIC
0.1,1.,0.05,1.
*BOUNDARY
DTOP,1,1,0.
*END STEP
********************