*HEADING
TEST DAMAGE INITIATION CONNECTOR AND CONNECTOR DAMAGE EVOLUTION BEHAVIORS - 3D - TEST DEGRADATION PARAMETER
*PREPRINT, MODEL=YES
**
***********************************************************
**		SECTION I: MODEL DATA
***********************************************************
**
*NODE
*ELEMENT, TYPE=CONN3D2, ELSET=C1
*CONNECTOR SECTION, ELSET=C1, BEHAVIOR=B1
CARTESIAN, CARDAN
GLOB
*ORIENTATION, NAME=GLOB
**
*CONNECTOR BEHAVIOR, NAME=B1
*INCLUDE, INPUT=misc_nonlinearelas_dam_conn3d.inp
*INCLUDE, INPUT=misc_plas_hard_conn3d.inp
*INCLUDE, INPUT=misc_dam_mult_degrad.inp
**
*ELEMENT, TYPE=MASS, ELSET=M1
*MASS, ELSET=M1
1E-3
*ELEMENT, TYPE=ROTARYI, ELSET=R1
*ROTARY INERTIA, ELSET=R1
1E-4, 1E-4, 1E-4
**
***********************************************************
**		SECTION II: HISTORY DATA
***********************************************************
**
*STEP
*DYNAMIC, EXPLICIT, DIRECT
1.0E-4, 1.0
*AMPLITUDE, NAME=CYCLE
0.0,0.0,1.0,1.0
*BOUNDARY
1,1,6,
*BOUNDARY, AMPLITUDE=CYCLE
2,1,6,1
*OUTPUT, HISTORY
*ELEMENT OUTPUT, ELSET=C1
CU, CUE, CUP, CUPEQ, CEF, CRF, CDIF, CDIM, CDIP, CDMG, CALPHAF
*END STEP