*HEADING
 USES DEPENDENCY FILE:  pca4gfsrf0
*PREPRINT,MODEL=YES,HIST=YES,ECH=YES
*RESTART,WRITE,FREQ=100
*SYMMETRIC RESULTS TRANSFER
*SYMMETRIC MODEL GENERATION,REVOLVE,NODEOFF=1000,ELEMENT=1000
 360, 6, 1.0, cylindrical
*****************************
*Step, name=Step-1, nlgeom, unsymm=yes
compress
*static
1., 1., 1E-05, 1.
*boundary
ASSEMBLY__G24, 2,2
*boundary,op=mod
ASSEMBLY__G26, 1, 1
ASSEMBLY__G26, 2, 2, -0.08
ASSEMBLY__G26, 3, 6
*restart, write, frequency=9999
*nset, nset=hs
*elset, elset=hs
*elset, elset=mm
*output, history, freq=5
*node output, nset=hs
u
*element output, elset=hs
s,le
*output, field, frequency=9999
*element output, elset=hs
s,le
*element output, elset=mm, rebar
s,le
*node output, nset=hs
u
*el file, frequency=9999, elset=hs
s,le
*el file, frequency=9999, elset=mm, rebar
s,le
*node file, frequency=9999, nset=hs
u
*endstep