*HEADING
 USES DEPENDENCY FILE:  pc38shmem1
*PREPRINT,MODEL=YES,HIST=YES,ECH=YES
*RESTART,WRITE,FREQ=100
*SYMMETRIC RESULTS TRANSFER
*SYMMETRIC MODEL GENERATION,REF=LIN,NODEOFF=100000,ELEMENT=100000
*****************************
*Step, inc=100, name=Step-1, nlgeom, unsymm=yes
compress
*static, direct
1., 1., 1E-05, 1.
*boundary
ASSEMBLY__G24, 2,2
*boundary,op=mod
ASSEMBLY__G26, 1, 1
ASSEMBLY__G26, 2, 2, -0.08
ASSEMBLY__G26, 3, 6
*restart, write, frequency=9999
*output, field, frequency=9999
*output, history, frequency=9999
*endstep
****************************
*step
remove constr 2
*static
1.0,1.0
*boundary, op=new
ASSEMBLY__G26, 1, 1
ASSEMBLY__G26, 2, 2, -0.08
ASSEMBLY__G26, 3, 6
*restart, write, frequency=9999
*nset, nset=hss
*elset, elset=hss
*elset, elset=mmm
*output, history, freq=5
*node output, nset=hss
u
*element output, elset=hss
s,le
*output, field, frequency=9999
*element output, elset=hss
s,le
*element output, elset=mmm, rebar
s,le
*node output, nset=hss
u
*el file, frequency=9999, elset=hss
s,le
*el file, frequency=9999, elset=mmm, rebar
s,le
*node file, frequency=9999, nset=hss
u
*endstep