*Heading
** Job name: spotweld_shear_coarse Model name: spotweld_shear_coarse
*Preprint, echo=NO, model=NO, history=NO, contact=NO
*Part, name=Part-1
*Include, input=spotweld_cm_part.inp
** Section: SteelSection
*Solid Section, elset=_PickedSet35, material=H340LAD
1.,
*End Part
**
**
** ASSEMBLY
**
*Assembly, name=Assembly
**
*Instance, name=Part-1-1, part=Part-1
*End Instance
**
*Node
*Node
*Node
*Element, type=CONN3D2
*Element, type=MASS, elset=Mass-1
*Element, type=ROTARYI, elset=Mass-2
*Elset, elset=Wire-1-Set-1
*Connector Section, elset=Wire-1-Set-1, behavior=ConnSect-1
Translator,
"Datum csys-2",
**
*Include, input=spotweld_cm_assembl.inp
**
*Surface, type=NODE, name=Fix-2_CNS_, internal
Fix-2, 1.
*Surface, type=NODE, name=Fix-1_CNS_, internal
Fix-1, 1.
*Orientation, name="Datum csys-2"
** Constraint: Constraint-1
*Coupling, constraint name=Constraint-1, ref node=Set-2, surface=Fix-2_CNS_
*Kinematic
** Constraint: Constraint-2
*Coupling, constraint name=Constraint-2, ref node=Set-1, surface=Fix-1_CNS_
*Kinematic
** QA Sets
*NSET, NSET=QA_TEST
Set-2
*ELSET, ELSET=QA_TEST
Part-1-1._PickedSet35
*End Assembly
*Mass, Elset=Mass-1
5.
*Rotary Inertia, Elset=Mass-2
500.
*Connector Behavior, name=ConnSect-1
*Connector Elasticity, component=1
*Amplitude, name=Amp-1, definition=SMOOTH STEP
0., 0., 10., 1.
*Include, input=spotweld_material.inp
**
** INTERACTION PROPERTIES
**
*Surface Interaction, name=IntProp-1
**
** BOUNDARY CONDITIONS
**
** Name: BC-1 Type: Displacement/Rotation
*Boundary
Set-2, 1,4
Set-2, 6, 6
** Name: BC-2 Type: Displacement/Rotation
*Boundary
Set-1, 1, 2
Set-1, 4, 6
** FIELD VARIABLE DEFINITION
*INITIAL CONDITIONS, TYPE=FIELD
ThermalZone2, 1.2
ThermalZone3, 1.0
ThermalZone1, 1.4
** ----------------------------------------------------------------
**
** STEP: Step-1
**
*Step, name=Step-1
*Dynamic, Explicit, element by element
, 50
*Bulk Viscosity
** Mass Scaling: Semi-Automatic
**               Whole Model
*Variable Mass Scaling, dt=0.001, type=below min, frequency=1
**
** BOUNDARY CONDITIONS
**
** Name: BC-3 Type: Velocity/Angular velocity
*Boundary, amplitude=Amp-1, type=VELOCITY
Set-3, 3, 3, -0.15
**
** INTERACTIONS
**
** Interaction: Int-1
*Contact, op=NEW
*Contact Inclusions, ALL EXTERIOR
*Contact property assignment
 ,  , IntProp-1
**
** OUTPUT REQUESTS
**
*Restart, write, number interval=1, time marks=NO
**
** FIELD OUTPUT: F-Output-1
**
*Output, field, number interval=10
*Node Output
U,
***Element Output, directions=YES
**DAMAGEC, DAMAGET, DMICRT, FV, LE, PE, PEEQ, S, SDEG, STATUS
***Contact Output
**CSTRESS,
**
** HISTORY OUTPUT: REF2
**
*Output, history
***Node Output, nset=Set-2
**RF1, RF2, RF3, RM, RM1, RM2, RM3
**U1, U2, U3, UR, UR1, UR2, UR3
**
** HISTORY OUTPUT: REF1
**
***Node Output, nset=Set-3
**RF1, RF2, RF3, RM, RM1, RM2, RM3
**U1, U2, U3, UR, UR1, UR2, UR3
**
** HISTORY OUTPUT:  QA Set
**
*Node Output, NSET=QA_TEST
RF3
**
** HISTORY OUTPUT: H-Output-1
**
*Energy Output, ELSET=QA_TEST
ALLAE,ALLCD,ALLDMD,ALLIE,ALLKE,ALLSE,ETOTAL
*End Step