*Heading
** Job name: src_rod_emc3d8 Model name: src_rod_emc3d8
** Generated by: Abaqus/CAE 6.12-DEV
*Preprint, echo=NO, model=NO, history=NO, contact=NO
**
** PARTS
**
*Part, name=problem_domain
*Node
*Element, type=EMC3D8
*Nset, nset=rod
*Elset, elset=rod, generate
*Nset, nset=coil
*Elset, elset=coil, generate
*Nset, nset=air
*Elset, elset=air
*Nset, nset=_PickedSet5, internal
*Elset, elset=_PickedSet5, internal
*Nset, nset=_PickedSet6, internal
*Elset, elset=_PickedSet6, internal, generate
** Section: air
*Solid Section, elset=_PickedSet5, material=air
** Section: conductor
*Solid Section, elset=_PickedSet6, material=conductor
*End Part
**
**
** ASSEMBLY
**
*Assembly, name=Assembly
**
*Instance, name=problem_domain-1, part=problem_domain
*End Instance
**
*Nset, nset=_PickedSet16, internal, instance=problem_domain-1
*Elset, elset=_PickedSet16, internal, instance=problem_domain-1, generate
*Elset, elset=_xzer_S5, internal, instance=problem_domain-1
*Elset, elset=_xzer_S4, internal, instance=problem_domain-1
*Elset, elset=_xzer_S3, internal, instance=problem_domain-1, generate
*Elset, elset=_xzer_S1, internal, instance=problem_domain-1, generate
*Elset, elset=_xzer_S2, internal, instance=problem_domain-1, generate
*Elset, elset=_xzer_S6, internal, instance=problem_domain-1, generate
*Surface, type=ELEMENT, name=xzer
_xzer_S5, S5
_xzer_S4, S4
_xzer_S2, S2
_xzer_S6, S6
_xzer_S3, S3
_xzer_S1, S1
*Elset, elset=_yzer_S2, internal, instance=problem_domain-1, generate
*Elset, elset=_yzer_S5, internal, instance=problem_domain-1
*Elset, elset=_yzer_S3, internal, instance=problem_domain-1
*Elset, elset=_yzer_S1, internal, instance=problem_domain-1, generate
*Elset, elset=_yzer_S4, internal, instance=problem_domain-1
*Elset, elset=_yzer_S6, internal, instance=problem_domain-1
*Surface, type=ELEMENT, name=yzer
_yzer_S2, S2
_yzer_S5, S5
_yzer_S4, S4
_yzer_S6, S6
_yzer_S3, S3
_yzer_S1, S1
*Elset, elset=_zzer_S4, internal, instance=problem_domain-1
*Elset, elset=_zzer_S6, internal, instance=problem_domain-1
*Elset, elset=_zzer_S3, internal, instance=problem_domain-1
*Elset, elset=_zzer_S5, internal, instance=problem_domain-1
*Elset, elset=_zzer_S2, internal, instance=problem_domain-1, generate
*Surface, type=ELEMENT, name=zzer
_zzer_S4, S4
_zzer_S6, S6
_zzer_S2, S2
_zzer_S3, S3
_zzer_S5, S5
*Elset, elset=_zpos_S3, internal, instance=problem_domain-1
*Elset, elset=_zpos_S6, internal, instance=problem_domain-1
*Elset, elset=_zpos_S5, internal, instance=problem_domain-1
*Elset, elset=_zpos_S4, internal, instance=problem_domain-1, generate
*Elset, elset=_zpos_S2, internal, instance=problem_domain-1, generate
*Surface, type=ELEMENT, name=zpos
_zpos_S3, S3
_zpos_S6, S6
_zpos_S4, S4
_zpos_S2, S2
_zpos_S5, S5
*Elset, elset=_outer_S6, internal, instance=problem_domain-1
*Elset, elset=_outer_S5, internal, instance=problem_domain-1
*Elset, elset=_outer_S4, internal, instance=problem_domain-1
*Elset, elset=_outer_S3, internal, instance=problem_domain-1, generate
*Surface, type=ELEMENT, name=outer
_outer_S6, S6
_outer_S5, S5
_outer_S4, S4
_outer_S3, S3
*Orientation, name=cyl, system=CYLINDRICAL
*End Assembly
**
** MATERIALS
**
*Material, name=air
*Electrical Conductivity
*Magnetic Permeability
*Material, name=conductor
*Electrical Conductivity
*Magnetic Permeability
** ----------------------------------------------------------------
**
** STEP: Step-1
**
*Step, name=Step-1, perturbation
*Electromagnetic, low frequency, time harmonic
**
** BOUNDARY CONDITIONS
**
** Name: far_field Type: Magnetic vector potential
*D EM Potential
outer, s, mvp, , 0., 0., 0., 0., 0., 0., 0., 0.
** Name: xsym Type: Magnetic vector potential
*D EM Potential
xzer, s, mvp, , 0., 0., 0., 0., 0., 0., 0., 0.
** Name: ysym Type: Magnetic vector potential
*D EM Potential
yzer, s, mvp, , 0., 0., 0., 0., 0., 0., 0., 0.
** Name: zpos Type: Magnetic vector potential
*D EM Potential
zpos, s, mvp, , 0., 0., 0., 0., 0., 0., 0., 0.
**
** LOADS
**
** Name: current   Type: Body current density
*Decurrent, real
_PickedSet16, CJ, 1e+07, 0., 1., 0., cyl
**
** OUTPUT REQUESTS
**
**
** FIELD OUTPUT: F-Output-1
**
*Output, field
*Element Output, directions=YES
EMB, EMBF, EMCD, EME, EMH, EMJH
*Output, history, frequency=0
*End Step