*HEADING
STD-STD IMPORT: TRANSFER OF TEMPERATURES
*IMPORT,UPDATE=YES,STATE=YES
EALL
*NODE,NSET=ALL1
*ELEMENT,TYPE=CPS4T,ELSET=TWO
*SOLID SECTION,ELSET=TWO,MATERIAL=A1
*NSET,NSET=LEFT1
*NSET,NSET=RIGHT1
*NSET,NSET=BOT1
*NSET,NSET=BOT
BOT,BOT1
*NSET,NSET=LEFT
LEFT,LEFT1
*NSET,NSET=TOP1
*INITIAL CONDITIONS, TYPE=TEMPERATURE
ALL1,25
*AMPLITUDE,NAME=STEP
0.0,1.0,1.0,1.0
*AMPLITUDE,NAME=NEW
0.0,0.0,1.0,2.0
*FILE FORMAT, ZERO INC
*STEP,NLGEOM,INC=20
*COUPLED TEMPERATURE-DISPLACEMENT
 0.1,1.0
*BOUNDARY, FIXED
 ALL,1,2
 ALL,11,11
*BOUNDARY
 LEFT1,1,2
 BOT1,2,2
 BOT1,11,11
 TOP1,11,11,50.0
*CLOAD,AMP=STEP
 RIGHT,1,1.0E7
*CLOAD
 RIGHT1,1,1.0E7
*ENERGY FILE
*OUTPUT,HISTORY,FREQUENCY=1
*ENERGY OUTPUT,VARIABLE=PRESELECT
*EL FILE
 S,EE,PE,THE
*OUTPUT,FIELD
*ELEMENT OUTPUT
 S,EE,PE,THE
*NODE OUTPUT
 NT,U
*NODE FILE
 NT,
*OUTPUT,FIELD
*NODE OUTPUT
RF,
NT,
RFL,
COORD,
*END STEP
*STEP,NLGEOM,INC=20
*COUPLED TEMPERATURE-DISPLACEMENT
 0.1,1.0
*BOUNDARY,OP=NEW
 LEFT,1,2
 BOT,2,2
 BOT,11,11
 TOP,11,11,100.0
 TOP1,11,11,100.0
*BOUNDARY,AMP=NEW, OP=NEW
 RIGHT,1,1,0.1
 RIGHT1,1,1,0.1
*ENDSTEP