*HEADING
Testing std-std import of rigid elements
and contact definitions
Second Standard Analysis
*IMPORT, STEP=1, UPDATE=NO, STATE=YES
 RIG, DEF
*IMPORT NSET
 REF, BOT, TOP
*PREPRINT, CONTACT=YES
*BOUNDARY
 999,1,6
*RESTART, WRITE
*FILE FORMAT, ZERO INCREMENT
*STEP, NLGEOM, INC=100
*STATIC
 0.1,1.0
*BOUNDARY
 TOP,1,1,5.0
*BOUNDARY,FIXED
 TOP,2,3
*EL FILE, ELSET=DEF
 S,LE
*NODE FILE
 U,
 COORD,
*ENERGY FILE
*CONTACT FILE
*OUTPUT, FIELD
*CONTACT OUTPUT
CSTRESS,CDISP
*ELEMENT OUTPUT
 S,LE
*NODE OUTPUT
 U,
 COORD,
*END STEP