*HEADING
 Transfer from Standard to Standard
 Test for S4R element with SHELL GENERAL SECTION
 - MATERIAL parameter included
 - shear test
*IMPORT,STEP=1,UPDATE=NO,STATE=YES
 SHELL,
*IMPORT NSET
 ALL,SIDE
*FILE FORMAT, ZERO INC
*RESTART, WRITE, FREQ=100
*NODE, NSET=ALL1
*NSET, NSET=SIDE1
*NODAL THICKNESS
*ELEMENT, TYPE=S4R, ELSET=SHELL1
*SHELL GENERAL SECTION, ELSET=SHELL1, POISSON=0., MATERIAL=STEL1,
ORIENTATION=SECOR, NODAL THICKNESS,CONTROLS=HGC
**
*STEP,NLGEOM,INC=50
*STATIC
 0.1, 1.
*BOUNDARY, FIXED
 ALL, 3,5
 1, 1,2
 2, 1,2
 3, 2,2
 4, 2,2
 3, 1, 1
 4, 1, 1
*BOUNDARY
 ALL1, 3,5
11, 1,2
12, 1,2
13, 2,2
14, 2,2
13, 1, 1, 1.0
14, 1, 1, 1.0
*EL FILE, DIRECTIONS=YES
S,
SF,
SE,
EE,
PE,
STH,
*NODE FILE
COORD,
*OUTPUT,FIELD,VARIABLE=PRESELECT
*ELEMENT OUTPUT
S,
SE
SF
EE,
PE,
STH,
*NODE OUTPUT
COORD
*END STEP