*HEADING
Testing Std-Std import of temperatures, field variables
*IMPORT,UPDATE=YES,STATE=YES,STEP=1
E1
*NODE,NSET=N3
*NSET,NSET=ALL
ALL,N3
*ELEMENT,TYPE=S4R,ELSET=E3
*SHELL SECTION,ELSET=E3,MATERIAL=A1,ORIENTATION=LOCAL1
0.1,
*ORIENTATION,NAME=LOCAL1
*INITIAL CONDITIONS,TYPE=TEMPERATURE
N3,-10.
*INITIAL CONDITIONS,TYPE=FIELD, VARIABLE=1
N3,5.0
*FILE FORMAT,ZERO INC
*STEP, NLGEOM
*STATIC
0.1,1.0
*TEMPERATURE
N1,200.,
N3,200.,
*FIELD,VARIABLE=1
N1,30.0
N3,30.0
*BOUNDARY,TYPE=VELOCITY
ALL,1,6
*OUTPUT,FIELD
*NODE OUTPUT
RF,
NT,
*OUTPUT,FIELD
*ELEMENT OUTPUT
 THE,
 S,
 LE,
 PE
*EL FILE
S,
THE,
LE,
EE
SINV
PE
FV
*NODE FILE
NT,
*ENDSTEP