*HEADING
 Transfer from Standard to Standard : elastic+plastic
 - Second Standard analysis
*IMPORT,UPDATE=NO,STATE=NO,STEP=1
ONE,
*RESTART, WRITE
*FILE FORMAT,ZERO INC
*STEP,NLGEOM
*DYNAMIC
0.01,0.1
*BOUNDARY,TYPE=VELOCITY
1,1,6
DISP,2,2
DISP,1,1,1.0
*NODE FILE
COORD,
*EL FILE
S,
EE,
LE,
PE,
*OUTPUT,FIELD,VARIABLE=PRESELECT,FREQ=1
*ELEMENT OUTPUT
S,
EE,
PE,
*NODE OUTPUT
COORD
*END STEP