*Heading
** Job name: gasket_sm Model name: Submodel
*Preprint, echo=NO, model=NO, history=NO, contact=NO
**
** PARTS
**
*Part, name=Gasket
*End Part
**
**
** ASSEMBLY
**
*Assembly, name=Assembly
**
*Instance, name=Gasket-1, part=Gasket
*Node
*Element, type=GK3D6
*Nset, nset=_PickedSet2, internal, generate
*Elset, elset=_PickedSet2, internal, generate
** Section: Gasket
*Gasket Section, elset=_PickedSet2, behavior=Gasket
*End Instance
**
*Nset, nset=_PickedSet27, internal, instance=Gasket-1, generate
*Elset, elset=_PickedSet27, internal, instance=Gasket-1, generate
*Elset, elset=_gasketTop_SPOS, internal, instance=Gasket-1, generate
*Surface, type=ELEMENT, name=gasketTop
_gasketTop_SPOS, SPOS
*Elset, elset=_gasketBottom_SNEG, internal, instance=Gasket-1, generate
*Surface, type=ELEMENT, name=gasketBottom
_gasketBottom_SNEG, SNEG
*Submodel, type=NODE, exteriorTolerance=0.05
_PickedSet27,
*End Assembly
**
** MATERIALS
**
*Gasket behavior, name=Gasket
*Gasket elasticity, component=MEMBRANE
*Gasket Thickness Behavior, type=DAMAGE
*Gasket elasticity
**
** INTERACTION PROPERTIES
**
*Surface Interaction, name=IntProp-1
1.,
** ----------------------------------------------------------------
**
** STEP: Step-1
**
*Step, name=Step-1, nlgeom=YES
*Static
1., 1., 1e-05, 1.
**
** BOUNDARY CONDITIONS
**
** Name: BC-3 Type: Submodel
*Boundary, submodel, step=1
_PickedSet27, 1, 1
_PickedSet27, 3, 3
**
** OUTPUT REQUESTS
**
*Restart, write, frequency=0
**
** FIELD OUTPUT: F-Output-1
**
*Output, field
*Node Output
U,
*Element Output, directions=YES
S,
**
** HISTORY OUTPUT: H-Output-1
**
*Output, history, variable=PRESELECT
*End Step