*HEADING
 Transfer from Standard to Explicit : Test for CAX4R element
 - Explicit analysis
 - further loading in shear
*IMPORT,STEP=1,UPDATE=YES,STATE=YES
 SHELL,
*IMPORT NSET
 ALL, SIDE
*NSET,NSET=all
*BOUNDARY
 1, 1,2
 2, 1,2
 3, 2,2
 4, 2,2
**
**
**
*NSET,NSET=TOP
*NSET, NSET=QA_TEST_ALLNODES
ALL,
*ELSET,ELSET=QA_TEST_ALLELEMS
SHELL,
*AMPLITUDE,NAME=AMP1,DEFINITION=SMOOTH
0,0,0.01,1.0
**
*STEP
*DYNAMIC,EXPLICIT
 , 0.01,
*BOUNDARY,TYPE=VELOCITY,AMPLITUDE=AMP1
TOP,1,1,5
*OUTPUT,FIELD,VARIABLE=PRESELECT
**FOR QA PURPOSE
*OUTPUT, FIELD, TIMEMARKS=YES, NUMBER INTERVAL=4
*ELEMENT OUTPUT,ELSET=QA_TEST_ALLELEMS
 LE,
*NODE OUTPUT,NSET=QA_TEST_ALLNODES
COORD,
*OUTPUT,HISTORY,TIME INTERVAL=0.001
*ENERGY OUTPUT
ALLIE,ALLKE,ALLSE,ALLWK,ETOTAL
*END STEP