*HEADING
 Transfer from Standard to Explicit: Test for cohesive elements
*PREPRINT, MODEL=YES
*IMPORT,STEP=1,UPDATE=NO,STATE=NO
COH3D8, COH3D6, COH2D4, COHAX4
*RESTART, WRITE
*BOUNDARY
 TOP_3D, 2, 2
 BOTTOM_3D, 1, 3
 TOP_2D, 2, 2
 BOTTOM_2D, 1, 2
*STEP
*DYNAMIC, EXPLICIT
, 0.2
*BOUNDARY
 15,1,1,0.0
 16,1,3,0.0
 17,3,3,0.0
 25,1,1,0.0
 26,1,3,0.0
 27,3,3,0.0
 33,1,,0.0
 43,1,,0.0
*OUTPUT,FIELD, NUMBER INTERVAL=10, TIME MARKS=YES
*ELEMENT OUTPUT
S, LE, NE,TSHR
*NODE OUTPUT
U,
*OUTPUT,HISTORY, TIME INTERVAL=0.01
*ENERGY OUTPUT
ALLSE, ALLKE, ALLDMD, ALLIE, ETOTAL, ALLWK
*END STEP