*HEADING
 Transfer from Standard to Explicit : MPC linear
 - Explicit analysis
 [references xs_s_cps4r_mpclin]
*IMPORT,UPDATE=NO,STATE=YES
ELALL,
*RESTART,TIMEMARKS=YES,WRITE,NUM=1
BOTTOM,2,2
*MPC
LINEAR,3,2,5
**
** STEP #1
**
**
*STEP
*DYNAMIC,EXPLICIT
,0.1
*BOUNDARY,TYPE=VELOCITY
LEFT,  1,1,
BOTTOM,2,2,
RIGHT, 1,1, 5.0
*FILE OUTPUT,TIMEMARKS=YES,NUM=1
*NODE FILE
U,
***OUTPUT,HISTORY,TIME INTERVAL=2.5E-3
***ELEMENT OUTPUT,ELSET=ELALL
**S,LE
*OUTPUT, FIELD, TIMEMARKS=YES, NUMBER INTERVAL=1
*NODE OUTPUT, NSET=QA_TEST_ALLNODES
U,
*OUTPUT,FIELD,VARIABLE=PRESELECT
*OUTPUT,HISTORY,VARIABLE=PRESELECT,TIMEINT=0.1
*END STEP