**
** test import of ductile damage evolution (type=ener, soft=lin)
** Standard to Explicit
**
*import,state=yes,update=no
 solid-2
**
*STEP,nlgeom=yes
*dynamic,explicit
 ,0.01
*BOUNDARY,TYPE=DISPLACEMENT
 y0,2,2
 x0,1,1
 z0,3,3
*boundary, type=velocity
 x1,1,1,1
**
**
*OUTPUT,FIELD,freq=10
*ELEMENT OUTPUT
 DMICRT
 PEEQ,
 S,
 PE
 SDEG
*NODE OUTPUT
 U,
*OUTPUT,HISTORY
*ELEMENT OUTPUT,ELSET=alle
 DMICRT
 PEEQ,
 MISES,
 PRESS,
 TRIAX,
 SDEG,
*END STEP