*HEADING
 Transfer from Standard to Explicit : Plasticity Test for T2D2 element
 - Explicit Analysis
 - Plastic material with combined hardening (multiple backstresses)
*IMPORT,STEP=2,UPDATE=NO,STATE=YES
 TRUSS,
*IMPORT NSET
 ALL,
*BOUNDARY
 1, 1,2
 1, 6,6
 2, 2,2
 2, 6,6
**
**
*ELSET, ELSET=QA_TEST_ALLELEMS
TRUSS,
**
*NSET, NSET=QA_TEST_ALLNODES
ALL,
**
*STEP,NLGEOM=YES
*DYNAMIC,EXPLICIT
 , 0.1
*BOUNDARY, TYPE=VELOCITY
 2, 1, 1, 0.08
*FILE OUTPUT,TIMEMARKS=YES, NUM=4
*EL FILE
 PEEQ,
 ALPHA
*NODE FILE
 U,
 COORD,
*OUTPUT, FIELD, TIMEMARKS=YES, NUMBER INTERVAL=4
*ELEMENT OUTPUT, ELSET=QA_TEST_ALLELEMS
 PEEQ, ALPHA
*NODE OUTPUT, NSET=QA_TEST_ALLNODES
 U,
 COORD,
*OUTPUT,FIELD,VARIABLE=PRESELECT
*OUTPUT,HISTORY,VARIABLE=PRESELECT,TIMEINT=0.025
***OUTPUT,HISTORY,VARIABLE=PRESELECT
*END STEP