********************************************************************
**           see tr_readme.inp for instructions
********************************************************************
**
**          parameters, materials
**
*include, input=tr_parameters_in_phase_db.inp
*include, input=tr_parameters_db.inp
*include, input=tr_materials_db.inp
**************************************************************
**------------------------------------------------
**
** PN = Chassis
**
*Part, name=Chassis
*Node
*************************************************
***Ref. nodes for chassis
*************************************************
**************************************************************
**reference node for RAIL-FRONT-OUTER-INNER-BACK-LEFT coupling
**************************************************************
**reference node for RAIL-FRONT-OUTER-INNER-BACK-RIGHT coupling
**************************************************************
*Element, type=S4R
*Element, type=B31
*Element, type=S3R
*Nset, nset=ALL_NODES
*Elset, elset=RAIL-FRONT-LEFT-INNER, generate
*Elset, elset=RAIL-FRONT-LEFT-OUTER, generate
*Elset, elset=RAIL-FRONT-RIGHT-INNER, generate
*Elset, elset=RAIL-FRONT-RIGHT-OUTER, generate
*Elset, elset=RAIL-BACK-LEFT, generate
*Elset, elset=RAIL-BACK-RIGHT, generate
*Elset, elset=RAIL-CONN-2, generate
*Elset, elset=RAIL-CONN-3, generate
*Elset, elset=RAIL-CONN-4, generate
*Elset, elset=SUSP_UPPER_ARM_LEFT_BRACKETS_BACK, generate
*Elset, elset=SUSP_UPPER_ARM_LEFT_BRACKETS_FRONT, generate
*Elset, elset=SUSP_UPPER_ARM_RIGHT_BRACKETS_FRONT, generate
*Elset, elset=SUSP_UPPER_ARM_RIGHT_BRACKETS_BACK, generate
*Elset, elset=SUSP_LOWER_ARM_LEFT_BRACKET_BACK
*Elset, elset=SUSP_LOWER_ARM_RIGHT_BRACKET_BACK
*Elset, elset=A-ARM-LOW-MTG-LEFT
*Elset, elset=A-ARM-LOW-MTG-RIGHT
*Elset, elset=SUSP_LOWER_ARM_LEFT_BRACKET_FRONT
*Elset, elset=SUSP_LOWER_ARM_RIGHT_BRACKET_FRONT
*Elset, elset=RADIATOR-MTG-M-LEFT, generate
*Elset, elset=RADIATOR-MTG-M-RIGHT, generate
*Elset, elset=CABIN-MTG-REINF-FRONT-LEFT, generate
*Elset, elset=CABIN-MTG-FRONT-RIGHT, generate
*Elset, elset=CABIN-MTG-REAR-LEFT, generate
*Elset, elset=CABIN-MTG-REAR-RIGHT, generate
*Elset, elset=ENGINE-CRADLE-LOW
*Elset, elset=ENGINE-CRADLE-UP, generate
*Elset, elset=RAIL-CON-5, generate
*Elset, elset=ENGINE-MOUNT-BOTTOM-LEFT, generate
*Elset, elset=ENGINE-MOUNT-BOTTOM-RIGHT, generate
*Elset, elset=ENGINE-MOUNT-BOTTOM2-RIGHT, generate
*Elset, elset=ENGINE-MOUNT-BOTTOM2-LEFT, generate
*Elset, elset=EVERYTHING_CHASSIS
*Elset, elset=EVERYTHING_ALL
*Elset, elset=BUMPER-MTG-FRONT-LT-RAIL, generate
*Elset, elset=BUMPER-MTG-FRONT-RT-RAIL, generate
*Elset, elset=BUMPER-MTG-S-LT-RAIL, generate
*Elset, elset=BUMPER-MTG-S-RT-RAIL
*Elset, elset=RADIATOR-MTG-M-LT-RAIL
*Elset, elset=RADIATOR-MTG-RT-RAIL
*Elset, elset=LOWER-ARM-LEFT-BRACKET-FRONT
*Elset, elset=LOWER-ARM-LEFT-BRACKET-BACK
*Elset, elset=LOWER-ARM-RIGHT-BRACKET-FRONT
*Elset, elset=LOWER-ARM-RIGHT-BRACKET-BACK
*Nset, nset=SUSP_UPPER_ARM_LEFT_BRACKET_BACK, generate
*Nset, nset=SUSP_UPPER_ARM_LEFT_BRACKET_BACK_RAIL
*Nset, nset=SUSP_UPPER_ARM_LEFT_BRACKET_FRONT
*Nset, nset=SUSP_UPPER_ARM_LEFT_BRACKET_FRONT_RAIL
*Nset, nset=SUSP_UPPER_ARM_RIGHT_BRACKET_FRONT, generate
*Nset, nset=SUSP_UPPER_ARM_RIGHT_BRACKET_FRONT_RAIL
*Nset, nset=SUSP_UPPER_ARM_RIGHT_BRACKET_BACK
*Nset, nset=SUSP_UPPER_ARM_RIGHT_BRACKET_BACK_RAIL
*Elset, elset=STABILIZER_CHASSIS_LEFT
*Elset, elset=STABILIZER_CHASSIS_RIGHT
*Elset, elset=RACK_CHASSIS
*Elset, elset=STRUT_CHASSIS_LEFT
*Elset, elset=STRUT_CHASSIS_RIGHT
*Elset, elset=ENGINE-MOUNT-BOTTOM2-LT
*Elset, elset=ENGINE-MOUNT-BOTTOM2-RT
*Elset, elset=ENGINE-MOUNT-REAR
*Elset, elset=CABIN-MTG-REINF-FRONT-RT-RAIL
*Elset, elset=CABIN-MTG-REINF-RIGHT-LT-RAIL
*Elset, elset=CABIN-MTG-REINF-RIGHT-RT-RAIL
*Elset, elset=CABIN-MTG-REINF-FRONT-LT-RAIL
*Elset, elset=RAIL-BACK-LT-BED-MTG-2
*Elset, elset=RAIL-BACK-LT-2-BED-MTG
*Elset, elset=RAIL-BACK-RT-1-BED-MTG
*Elset, elset=RAIL-BACK-RT-2-BED-MTG
*Elset, elset=RAIL-MTG-3-RAIL-LT-BED
*Elset, elset=RAIL-MTG-3-RAIL-RT-BED
*Elset, elset=RAIL-MTG-4-RAIL-LT-BED
*Elset, elset=RAIL-MTG-4-RAIL-RT-BED
*Elset, elset=RAIL-FRONT-OUTER-INNER-BACK-RIGHT
*Elset, elset=RAIL-FRONT-OUTER-INNER-BACK-LEFT
*Elset, elset=LEFT-REAR-SUSP-FRONT
*Elset, elset=LEFT-REAR-SUSP-BACK
*Elset, elset=RIGHT-REAR-SUSP-FRONT
*Elset, elset=RIGHT-REAR-SUSP-BACK
*Elset, elset=CHASSIS-FUEL-TANK1
*Elset, elset=CHASSIS-FUEL-TANK2
*Elset, elset=CHASSIS-FUEL-TANK3
*Elset, elset=CHASSIS-FUEL-TANK4
*Elset, elset=_BUMPER-MTG-FRONT-LT-RAIL_SPOS, internal, generate
*Elset, elset=_BUMPER-MTG-FRONT-RT-RAIL_SPOS, internal, generate
*Elset, elset=_BUMPER-MTG-S-LT-RAIL_SPOS, internal, generate
*Elset, elset=_BUMPER-MTG-S-RT-RAIL_SPOS, internal
*Elset, elset=_RADIATOR-MTG-M-LT-RAIL_SPOS, internal
*Elset, elset=_RADIATOR-MTG-RT-RAIL_SPOS, internal
*Elset, elset=_LOWER-ARM-LEFT-BRACKET-FRONT_SPOS, internal
*Elset, elset=_LOWER-ARM-LEFT-BRACKET-BACK_SPOS, internal
*Elset, elset=_LOWER-ARM-RIGHT-BRACKET-FRONT_SPOS, internal
*Elset, elset=_LOWER-ARM-RIGHT-BRACKET-BACK_SPOS, internal
*Elset, elset=_SUSP-UPPER-ARM-LEFT-BRACKETS-BACK_SPOS, internal, generate
*Elset, elset=_SUSP-UPPER-ARM-LEFT-BRACKETS-FRONT_SPOS, internal, generate
*Elset, elset=_SUSP-UPPER-ARM-RIGHT-BRACKETS-FRONT_SPOS, internal, generate
*Elset, elset=_SUSP-UPPER-ARM-RIGHT-BRACKETS-BACK_SPOS, internal, generate
*Elset, elset=_STABILIZER_CHASSIS_LEFT_SPOS, internal
*Elset, elset=_STABILIZER_CHASSIS_RIGHT_SPOS, internal
*Elset, elset=_RACK_CHASSIS_SPOS, internal
*Elset, elset=_STRUT_CHASSIS_LEFT_SPOS, internal
*Elset, elset=_STRUT_CHASSIS_RIGHT_SPOS, internal
*Elset, elset=_ENGINE-MOUNT-BOTTOM2-LT_SNEG, internal
*Elset, elset=_ENGINE-MOUNT-BOTTOM2-RT_SNEG, internal
*Elset, elset=_ENGINE-MOUNT-REAR_SPOS, internal
*Elset, elset=_CABIN-MTG-REINF-FRONT-RT-RAIL_SPOS, internal
*Elset, elset=_CABIN-MTG-REINF-RIGHT-LT-RAIL_SPOS, internal
*Elset, elset=_CABIN-MTG-REINF-RIGHT-RT-RAIL_SPOS, internal
*Elset, elset=_CABIN-MTG-REINF-FRONT-LT-RAIL_SPOS, internal
*Elset, elset=_RAIL-BACK-LT-BED-MTG-2_SPOS, internal
*Elset, elset=_RAIL-BACK-LT-2-BED-MTG_SPOS, internal
*Elset, elset=_RAIL-BACK-RT-1-BED-MTG_SPOS, internal
*Elset, elset=_RAIL-BACK-RT-2-BED-MTG_SPOS, internal
*Elset, elset=_RAIL-MTG-3-RAIL-LT-BED_SPOS, internal
** 48881, 48882, 48883, 48884, 48885, 48913, 48914, 48915, 48916, 48917,
*Elset, elset=_RAIL-MTG-3-RAIL-RT-BED_SPOS, internal
** 23009, 23010, 23011, 23012, 23013,  23041, 23042, 23043, 23044, 23045
*Elset, elset=_RAIL-MTG-4-RAIL-LT-BED_SPOS, internal
*Elset, elset=_RAIL-MTG-4-RAIL-RT-BED_SPOS, internal
**22997, 22998, 22999, 23029, 23000, 23030, 23031, 23032,
*Elset, elset=_RAIL-FRONT-OUTER-INNER-BACK-RIGHT_SPOS, internal
*Elset, elset=_RAIL-FRONT-OUTER-INNER-BACK-LEFT_SPOS, internal
*Elset, elset=_LEFT-REAR-SUSP-FRONT_SPOS, internal
*Elset, elset=_LEFT-REAR-SUSP-BACK_SPOS, internal
** 48685, 48686, 48687, 48688, 48689, 48690, 48691, 48692, 48717, 48718, 48719, 48720, 48721, 48722, 48723, 48724
** 48750, 48751, 48752, 48753, 48754, 48755, 48756, 48757, 48783, 48784, 48785, 48786, 48787, 48788, 48789, 48790
** 48816, 48817, 48818, 48819, 48820, 48821, 48822, 48823, 48824, 48825, 48826, 48827, 48828, 48829, 48830, 48831
*Elset, elset=_RIGHT-REAR-SUSP-FRONT_SPOS, internal
*Elset, elset=_RIGHT-REAR-SUSP-BACK_SPOS, internal
** 22813, 22814, 22815, 22816, 22817, 22818, 22819, 22820, 22847, 22848, 22849, 22850, 22851, 22852
** 22880, 22881, 22882, 22883, 22884, 22885, 22913, 22914, 22915, 22916, 22917, 22918, 22946,
** 22947, 22948, 22949, 22950, 22951, 22952, 22953, 22954, 22955, 22956, 22957
*Elset, elset=_CHASSIS-FUEL-TANK1_SPOS, internal
*Elset, elset=_CHASSIS-FUEL-TANK2_SPOS, internal
*Elset, elset=_CHASSIS-FUEL-TANK3_SPOS, internal
*Elset, elset=_CHASSIS-FUEL-TANK4_SPOS, internal
*ELEMENT, TYPE=MASS, ELSET=chassis_mass
*MASS, ELSET=chassis_mass
1.e-6,
*ELEMENT, TYPE=ROTARYI, ELSET=chassis_rotary
*ROTARY INERTIA, ELSET=chassis_rotary
1.e-6,1.e-6,1.e-6
*End Part
**------------------------------------------------
**
** PART = Bed
**
*Part, name=Bed
*Node
***Ref nodes
**
** 1900762,  1.603407e+003,  6.041082e+002,  4.866398e+002
**
*Element, type=S4R
*Element, type=B31
*Element, type=S3R
*Nset, nset=ALL_NODES
*Elset, elset=BED-OUTER, generate
*Elset, elset=BED-MTG-1-LEFT, generate
*Elset, elset=BED-MTG-1-RIGHT, generate
*Elset, elset=BED-MTG-2-LEFT, generate
*Elset, elset=BED-MTG-2-RIGHT, generate
*Elset, elset=BED-FENDER-STIFF, generate
*Elset, elset=BED-MTG-1-LT-BED
*Elset, elset=BED-MTG-1-LT-MTG
*Elset, elset=BED-MTG-1-RT-BED
*Elset, elset=BED-MTG-1-RT-MTG
*Elset, elset=BED-MTG-2-LT-BED
*Elset, elset=BED-MTG-2-LT-MTG
*Elset, elset=BED-MTG-2-RT-BED
*Elset, elset=BED-MTG-2-RT-MTG
*Elset, elset=BED-MTG-1-RAIL-LT-RAIL
*Elset, elset=BED-MTG-2-RAIL-LT-RAIL, generate
*Elset, elset=BED-MTG-1-RAIL-RT-RAIL
*Elset, elset=BED-MTG-2-RAIL-RT-RAIL, generate
*Elset, elset=BED-MTG-3-RAIL-LT-RAIL
*Elset, elset=BED-MTG-3-RAIL-RT-RAIL
*Elset, elset=BED-MTG-4-RAIL-LT-RAIL
*Elset, elset=BED-MTG-4-RAIL-RT-RAIL
*Elset, elset=EVERYTHING_BED
*Elset, elset=EVERYTHING_ALL
*Elset, elset=_BED-MTG-1-LT-SUR_SPOS, internal
*Elset, elset=_BED-MTG-1-LT-MTG-SUR_SPOS, internal
*Elset, elset=_BED-MTG-1-RT-BED-SUR_SPOS, internal
*Elset, elset=_BED-MTG-1-RT-MTG-SUR_SPOS, internal
*Elset, elset=_BED-MTG-2-LT-BED-SUR_SPOS, internal
*Elset, elset=_BED-MTG-2-LT-MTG-SUR_SPOS, internal
*Elset, elset=_BED-MTG-2-RT-BED-SUR_SPOS, internal
*Elset, elset=_BED-MTG-2-RT-MTG-SUR_SPOS, internal
*Elset, elset=_BED-MTG-1-RAIL-LT-RAIL_SPOS, internal
*Elset, elset=_BED-MTG-2-RAIL-LT-RAIL_SPOS, internal, generate
*Elset, elset=_BED-MTG-1-RAIL-RT-RAIL_SPOS, internal
*Elset, elset=_BED-MTG-2-RAIL-RT-RAIL_SPOS, internal, generate
*Elset, elset=_BED-MTG-3-RAIL-LT-RAIL_SPOS, internal
*Elset, elset=_BED-MTG-3-RAIL-RT-RAIL_SPOS, internal
*Elset, elset=_BED-MTG-4-RAIL-LT-RAIL_SPOS, internal
*Elset, elset=_BED-MTG-4-RAIL-RT-RAIL_SPOS, internal
*ELEMENT, TYPE=MASS, ELSET=bed_mass
*MASS, ELSET=bed_mass
1.e-6,
*ELEMENT, TYPE=ROTARYI, ELSET=bed_rotary
*ROTARY INERTIA, ELSET=bed_rotary
1.e-6,1.e-6,1.e-6
**--------------------------------------------------------
*nset,nset=retained_bed,unsorted
*nset,nset=retained_all
retained_bed,
*End Part
**------------------------------------------------
***
**
** PART = Fuel Tank
**
*Part, name=Fuel_Tank
*Node
**
***Ref Node
**
**
***Connector Node
**
**
*Element, type=S4R
*Element, type=S3R
*Nset, nset=ALL_NODES
*Elset, elset=FUEL_TANK, generate
*Elset, elset=FUEL_TANK_STRIPES, generate
*Elset, elset=EVERYTHING_FUEL_TANK, generate
*Elset, elset=EVERYTHING_ALL, generate
*Elset, elset=FUEL-TANK1
*Elset, elset=FUEL-TANK2
*Elset, elset=FUEL-TANK3
*Elset, elset=FUEL-TANK4
*Elset, elset=_FUEL-TANK1_SPOS, internal
*Elset, elset=_FUEL-TANK2_SPOS, internal
*Elset, elset=_FUEL-TANK3_SPOS, internal
*Elset, elset=_FUEL-TANK4_SPOS, internal
*ELEMENT, TYPE=MASS, ELSET=fuel_tank_mass
*MASS, ELSET=fuel_tank_mass
1.e-6,
*ELEMENT, TYPE=ROTARYI, ELSET=fuel_tank_rotary
*ROTARY INERTIA, ELSET=fuel_tank_rotary
1.e-6,1.e-6,1.e-6
*nset,nset=retained_fuel_tank,unsorted
*nset,nset=retained_all
retained_fuel_tank,
**
**
*End Part
**------------------------------------------------
**
** PART = Bumper
**
*Part, name=Bumper
*Node
**
***Ref Node
**
**
***Connector Node
**
**
*Element, type=S3R
*Element, type=S4R
*Nset, nset=ALL_NODES
*Elset, elset=BUMPER, generate
*Elset, elset=BUMPER-MTG-FRONT-LEFT, generate
*Elset, elset=BUMPER-MTG-FRONT-RIGHT, generate
*Elset, elset=BUMPER-MTG-S-LEFT, generate
*Elset, elset=BUMPER-MTG-S-RIGHT, generate
*Elset, elset=EVERYTHING_BUMPER, generate
*Elset, elset=EVERYTHING_ALL, generate
*Elset, elset=BUMPER-MTG-FRONT-LT
*Elset, elset=BUMPER-MTG-S-LT
*Elset, elset=BUMPER-MTG-FRONT-RT
*Elset, elset=BUMPER-MTG-S-RT, generate
*Elset, elset=_BUMPER-MTG-FRONT-LT_SPOS, internal
*Elset, elset=_BUMPER-MTG-S-LT_SPOS, internal
*Elset, elset=_BUMPER-MTG-FRONT-RIGHT_SPOS, internal
*Elset, elset=_BUMPER-MTG-S-RT_SPOS, internal, generate
*ELEMENT, TYPE=MASS, ELSET=bumper_mass
*MASS, ELSET=bumper_mass
1.e-6,
*ELEMENT, TYPE=ROTARYI, ELSET=bumper_rotary
*ROTARY INERTIA, ELSET=bumper_rotary
1.e-6,1.e-6,1.e-6
*nset,nset=retained_bumper,unsorted
*nset,nset=retained_all
retained_bumper
*End Part
**------------------------------------------------
**
** PARTS
**
**
*Part, name=Cabin
*Node
*******end of dashboard nodes
*** Ref. nodes
******COUPLING REF NODE FOR DOOR FRAME BOTTOM LEFT*****
******COUPLING REF NODE FOR DOOR FRAME BOTTOM RIGHT*****
********************************************************
******COUPLING REF NODE FOR DOOR FRAME UP RIGHT*********
********************************************************
**
*****************************************************
******COUPLING REF NODE FOR DOOR FRAME UP LEFT*****
**
****
*************************************************
****MPC REFERENCE NODE FOR RADIATOR TOP-2
******BL
*****BR
*****TL
****TR
**
********************************************************
*Element, type=C3D8R
*Element, type=S4R
*Element, type=S3R
*Nset, nset=ALL_NODES
*Elset, elset=FENDER-INNER-LEFT, generate
*Elset, elset=FENDER-INNER-RIGHT, generate
*Elset, elset=FENDER-OUTER-LEFT, generate
*Elset, elset=FENDER-OUTER-RIGHT, generate
*Elset, elset=FENDER-MTG-LEFT, generate
*Elset, elset=FENDER-MTG-RIGHT, generate
*Elset, elset=FENDER-MTG-UP-LEFT, generate
*Elset, elset=FENDER-MTG-UP-RIGHT, generate
*Elset, elset=WHEELHOUSE-LEFT, generate
*Elset, elset=WHEELHOUSE-RIGHT, generate
*Elset, elset=RADIATOR-MTG, generate
*Elset, elset=RAD-MTG-TOP-2, generate
*Elset, elset=RAD-MTG-TOP, generate
*Elset, elset=RAD-MTG-SIDE, generate
*Elset, elset=RAD-MTG-MIDDLE, generate
*Elset, elset=RAD-MTG-BRACKET, generate
*Elset, elset=RAD-MTG-BOT-UNDER, generate
*Elset, elset=RAD-MTG-BOT
*Elset, elset=RADIATOR, generate
*Elset, elset=RADIATOR-1, generate
*Elset, elset=RADIATOR-RIMMS, generate
*Elset, elset=RADIATOR-SIDE, generate
*Elset, elset=RADIATOR-SIDE-BL, generate
*Elset, elset=FAN-COVER-LOW, generate
*Elset, elset=FAN-COVER-TOP, generate
*Elset, elset=CABIN-BOTTOM-CENTER, generate
*Elset, elset=CABIN-BOTTOM-LEFT
*Elset, elset=CABIN-BOTTOM-RIGHT
*Elset, elset=CABIN-ROOF-INNER, generate
*Elset, elset=CABIN-ROOF-OUTER, generate
*Elset, elset=CABIN-BACK-PILLAR-LOW-LEFT, generate
*Elset, elset=CABIN-BACK-PILLAR-OUTER-LEFT, generate
*Elset, elset=CABIN-BACK-PILLAR-OUTER-RIGHT, generate
*Elset, elset=CABIN-BACK-PILLAR-UP-LEFT, generate
*Elset, elset=CABIN-BACK-PILLAR-UP-RIGHT, generate
*Elset, elset=CABIN-FIREWALL, generate
*Elset, elset=CABIN-FIREWALL-SIDE-LEFT, generate
*Elset, elset=CABIN-FIREWALL-SIDE-RIGHT, generate
*Elset, elset=CABIN-DASHBOARD-UP, generate
*Elset, elset=CABIN-WINDOW-FIX, generate
*Elset, elset=CABIN-BACK, generate
*Elset, elset=CABIN-BACK-REINF, generate
*Elset, elset=CABIN-DOORJAMP-LEFT, generate
*Elset, elset=CABIN-DOORJAMP-RIGHT, generate
*Elset, elset=CABIN-MTG-REINF-RIGHT-LEFT, generate
*Elset, elset=CABIN-MTG-REINF-RIGHT-RIGHT, generate
*Elset, elset=CABIN-D-HINGE-UP-LEFT, generate
*Elset, elset=CABIN-D-HINGE-UP-RIGHT, generate
*Elset, elset=CABIN-D-HINGE-LOW-LEFT, generate
*Elset, elset=CABIN-D-HINGE-LOW-RIGHT, generate
*Elset, elset=CABIN-BACK-PILLAR-LOW-RIGHT, generate
*Elset, elset=WINDOW-FRONT, generate
*Elset, elset=WINDOW-BACK, generate
*Elset, elset=DASHBOARD-INTERIOR
*Elset, elset=BATTERY, generate
*Elset, elset=BATTERY-TRAY-SIDE, generate
*Elset, elset=BATTERY-TRAY-TOP, generate
*Elset, elset=STEER-SUPPORT-TOP, generate
*Elset, elset=STEER-SUPPORT-LOW
*Elset, elset=STEER-DASH-SUPP
*Elset, elset=RADIATOR-OUTER, generate
*Elset, elset=STEER-COLUMN, generate
*Elset, elset=ACCELEROMETER-CG
*Elset, elset=HOOD-HINGE-1-LEFT, generate
*Elset, elset=HOOD-HINGE-1-RIGHT, generate
*Elset, elset=HOOD-HINGE-2-LEFT, generate
*Elset, elset=HOOD-HINGE-2-RIGHT, generate
*Elset, elset=DOOR-CLOSURE-IN-LEFT, generate
*Elset, elset=DOOR-CLOSURE-IN-RIGHT, generate
*Nset, nset=RADIATOR-BL, generate
*Nset, nset=RADIATOR-BR, generate
*Nset, nset=RADIATOR-TL, generate
*Nset, nset=RADIATOR-TR, generate
*Elset, elset=CABIN-D-HINGE-UP-LT
*Elset, elset=CABIN-D-HINGE-LOW-LT
*Elset, elset=CABIN-DOORJAMP-LT, generate
*Elset, elset=CABIN-D-HINGE-UP-RT
*Elset, elset=CABIN-D-HINGE-LOW-RT
*Elset, elset=CABIN-DOORJAMP-RT
*Elset, elset=CABIN-MTG-REINF-FRONT-LT, generate
*Elset, elset=CABIN-MTG-REINF-FRONT-RT, generate
*Elset, elset=CABIN-MTG-REINF-RIGHT-LT, generate
*Elset, elset=CABIN-MTG-REINF-RIGHT-RT, generate
*Elset, elset=RADIATOR-MTG-M-LT, generate
*Elset, elset=RADIATOR-MTG-M-RT, generate
*Elset, elset=HOOD-HINGE-2-LT
*Elset, elset=HOOD-HINGE-2-RT
*Elset, elset=HOOD-AXIAL-CONN
*Nset, nset=NODESET-34
*Nset, nset=NODESET-47
*Elset, elset=SEAT-TRK-FRONT-RT-CABIN-BOT
*Elset, elset=SEAT-TRK-REAR-RT-CABIN-BOT
*Elset, elset=SEAT-TRK-FRONT-LT-CABIN-BOT
*Elset, elset=SEAT-TRK-REAR-LT-CABIN-BOT
*Elset, elset=EVERYTHING_CABIN
*Elset, elset=EVERYTHING_ALL
*ELEMENT, TYPE=B31, ELSET=RAD-MTG-BEAMS
*ELEMENT, TYPE=B31, ELSET=DASHBOARD-SUPPORT
*Elset, elset=_CABIN-D-HINGE-UP-LT_SNEG, internal, generate
*Elset, elset=_CABIN-D-HINGE-LOW-LT_SNEG, internal, generate
*Elset, elset=_DOOR-CLOSURE-IN-LT_SNEG, internal, generate
*Elset, elset=_CABIN-DOORJAMP-LT_SNEG, internal, generate
*Elset, elset=_CABIN-D-HINGE-UP-RT_SNEG, internal, generate
*Elset, elset=_CABIN-D-HINGE-LOW-RT_SNEG, internal, generate
*Elset, elset=_CABIN-DOORJAMP-RT_SNEG, internal
*Elset, elset=_DOOR-CLOSURE-IN-RT_SPOS, internal, generate
*Elset, elset=_CABIN-MTG-REINF-FRONT-LT_SPOS, internal, generate
*Elset, elset=_CABIN-MTG-REINF-FRONT-RT_SPOS, internal, generate
*Elset, elset=_CABIN-MTG-REINF-RIGHT-LT_SPOS, internal, generate
*Elset, elset=_CABIN-MTG-REINF-RIGHT-RT_SPOS, internal, generate
*Elset, elset=_RADIATOR-MTG-M-LT_SPOS, internal, generate
*Elset, elset=_RADIATOR-MTG-M-RT_SPOS, internal, generate
*Elset, elset=_HOOD-HINGE-2-LT_SPOS, internal
*Elset, elset=_HOOD-HINGE-2-RT_SPOS, internal
*Elset, elset=_HOOD-AXIAL-CONN_SPOS, internal
*Elset, elset=_STEER-COLUMN_SPOS, internal, generate
*Elset, elset=_ACCELEROMETER-CG_S2, internal
*Elset, elset=_SEAT-TRK-FRONT-RT-CABIN-BOT_SPOS, internal
*Elset, elset=_SEAT-TRK-REAR-RT-CABIN-BOT_SPOS, internal
*Elset, elset=_SEAT-TRK-FRONT-LT-CABIN-BOT_SPOS, internal
*Elset, elset=_SEAT-TRK-REAR-LT-CABIN-BOT_SPOS, internal
*ELEMENT, TYPE=MASS, ELSET=cabin_mass
*MASS, ELSET=cabin_mass
1e-6,
*ELEMENT, TYPE=ROTARYI, ELSET=cabin_rotary
*ROTARY INERTIA, ELSET=cabin_rotary
1.e-6,1.e-6,1.e-6
**--------------------------------------------------------
****************************************************************************
*nset,nset=retained_cabin_chassis,unsorted
*nset,nset=retained_cabin_radiator_chassis,unsorted
*nset,nset=retained_cabin_door_left,unsorted
*nset,nset=retained_cabin_door_right,unsorted
*nset,nset=retained_cabin_hood,unsorted
*nset,nset=retained_cabin_seat,unsorted
*nset,nset=retained_cabin_cg
**
*nset,nset=retained_cabin,unsorted
*nset,nset=retained_all
retained_cabin, 2990460, 3990460,
*End Part
**------------------------------------------------
**
** PART = Seat
**
*Part, name=Seat
*Node
***Ref. nodes
*Element, type=C3D8R
*Element, type=B31
*Element, type=S4R
*Element, type=S3R
*Nset, nset=ALL_NODES
*Elset, elset=SEAT-HEADREST, generate
*Elset, elset=SEAT-BOTTOM, generate
*Elset, elset=SEAT-TOP, generate
*Elset, elset=SEAT-TRACK, generate
*Elset, elset=HEADREST-CONN-BEAMS, generate
*Elset, elset=EVERYTHING_SEAT
*Elset, elset=EVERYTHING_ALL
*ELEMENT, TYPE=MASS, ELSET=seat_mass
*MASS, ELSET=seat_mass
1.e-6,
*ELEMENT, TYPE=ROTARYI, ELSET=seat_rotary
*ROTARY INERTIA, ELSET=seat_rotary
1.e-6,1.e-6,1.e-6
**-----------------------------------------------------
*nset,nset=retained_seat,unsorted
*nset,nset=retained_all
retained_seat,
*NSET,NSET=SEAT_TRK_LT_889
*NSET,NSET=SEAT_TRK_LT_890
*NSET,NSET=SEAT_TRK_RT_891
*NSET,NSET=SEAT_TRK_RT_892
*End Part
**------------------------------------------------
**
** PART = Left_Door
**
*Part, name=Left_Door
*Node
**
***Ref Node
**
**
***Connector Node
**
**
*Element, type=C3D8R
*Element, type=B31
*Element, type=S4R
*Element, type=S3R
*Nset, nset=ALL_NODES
*Elset, elset=DOOR-CLOSURE-LEFT, generate
*Elset, elset=DOOR-INNER-LEFT, generate
*Elset, elset=DOOR-OUTER-LEFT, generate
*Elset, elset=DOOR-SIDEB-LEFT, generate
*Elset, elset=DOOR-SIDEBAR-REINF-LEFT, generate
*Elset, elset=DOOR-SIDEB-MTG1-LEFT
*Elset, elset=DOOR-SIDEB-MTG3-LEFT
*Elset, elset=DOOR-SIDEB-ST1-LEFT, generate
*Elset, elset=DOOR-TOPBAR-INN-LEFT, generate
*Elset, elset=DOOR-TOPBAR-OUT-LEFT, generate
*Elset, elset=DOOR-WINDOWWG-LEFT, generate
*Elset, elset=DOOR-REINF-LEFT, generate
*Elset, elset=DOOR-HINGE-LOW-LEFT, generate
*Elset, elset=DOOR-HINGE-UP-LEFT, generate
*Elset, elset=DOOR-LOCK-LEFT, generate
*Elset, elset=WINDOW-SIDE-LEFT, generate
*Elset, elset=DOOR-LOCK-BEAM-LEFT, generate
*Elset, elset=EVERYTHING_DOOR_LEFT
*Elset, elset=EVERYTHING_ALL
*Nset, nset=DOOR-LOCK-BEAMS-LT-COUP-1
*Nset, nset=DOOR-LOCK-LT-COUP-1, generate
*Nset, nset=DOOR-LOCK-LT-COUP
*Elset, elset=_DOOR-HINGE-LOW-LT-COUP_SPOS, internal, generate
*Elset, elset=_DOOR-HINGE-UP-LT-COUP_SPOS, internal, generate
*Elset, elset=_DOOR-CLOSURE-LEFT_SPOS, internal, generate
*ELEMENT, TYPE=MASS, ELSET=door_left_mass
*MASS, ELSET=door_left_mass
1.e-6,
*ELEMENT, TYPE=ROTARYI, ELSET=door_left_rotary
*ROTARY INERTIA, ELSET=door_left_rotary
1.e-6,1.e-6,1.e-6
*nset,nset=retained_door_left,unsorted
*nset,nset=retained_all
retained_door_left,
**
*End Part
**------------------------------------------------
**
** PART = Right_Door
**
*Part, name=Right_Door
*Node
**
***Ref Node
**
**
***Connector Node
**
**
*Element, type=C3D8
*Element, type=B31
*Element, type=S4R
*Element, type=S3R
*Nset, nset=ALL_NODES
*Elset, elset=DOOR-CLOSURE-RIGHT, generate
*Elset, elset=DOOR-INNER-RIGHT, generate
*Elset, elset=DOOR-OUTER-RIGHT, generate
*Elset, elset=DOOR-SIDEBAR-RIGHT, generate
*Elset, elset=DOOR-SIDEBAR-REINF-RIGHT, generate
*Elset, elset=DOOR-SIDEB-MTG1-RIGHT
*Elset, elset=DOOR-SIDEB-MTG3-RIGHT
*Elset, elset=DOOR-SIDEB-ST1-RIGHT, generate
*Elset, elset=DOOR-TOPBAR-INN-RIGHT, generate
*Elset, elset=DOOR-TOPBAR-OUT-RIGHT, generate
*Elset, elset=DOOR-WINDOWG-RIGHT, generate
*Elset, elset=DOOR-REINF-RIGHT, generate
*Elset, elset=DOOR-HINGE-LOW-RIGHT, generate
*Elset, elset=DOOR-HINGE-UP-RIGHT, generate
*Elset, elset=DOOR-LOCK-RIGHT, generate
*Elset, elset=WINDOW-SIDE-RIGHT, generate
*Elset, elset=DOOR-LOCK-RIGHT-BEAM, generate
*Elset, elset=EVERYTHING_DOOR_RIGHT
*Elset, elset=EVERYTHING_ALL
*Nset, nset=DOOR-LOCK-BEAMS-RT-COUP-1
*Nset, nset=DOOR-LOCK-RT-COUP-1, generate
*Nset, nset=DOOR-LOCK-RT-COUP
*Elset, elset=_DOOR-HINGE-LOW-RIGHT_SPOS, internal, generate
*Elset, elset=_DOOR-HINGE-UP-RIGHT_SPOS, internal, generate
*Elset, elset=_DOOR-CLOSURE-RIGHT_SPOS, internal, generate
*ELEMENT, TYPE=MASS, ELSET=door_right_mass
*MASS, ELSET=door_right_mass
1.e-6,
*ELEMENT, TYPE=ROTARYI, ELSET=door_right_rotary
*ROTARY INERTIA, ELSET=door_right_rotary
1.e-6,1.e-6,1.e-6
*nset,nset=retained_door_right,unsorted
*nset,nset=retained_all
retained_door_right,
**
*End Part
**------------------------------------------------
**
** PART = Hood
**
*Part, name=Hood
*Node
**
***Ref Node
**
**
***Connector Node
**
**
*Element, type=S4R
*Element, type=S3R
*Nset, nset=ALL_NODES
*Elset, elset=HOOD-INNER, generate
*Elset, elset=HOOD-OUTER, generate
*Elset, elset=EVERYTHING_HOOD
*Elset, elset=EVERYTHING_ALL
*Elset, elset=HOOD-LEFT-CONN
*Elset, elset=HOOD-RIGHT-CONN
*Elset, elset=HOOD-LOCK
*Elset, elset=_HOOD-FENDER-CONN_SPOS, internal
*Elset, elset=_HOOD-FENDER-CONN-RT_SPOS, internal
*Elset, elset=_HOOD-LOCK_SPOS, internal
*ELEMENT, TYPE=MASS, ELSET=hood_mass
*MASS, ELSET=hood_mass
1.e-6,
*ELEMENT, TYPE=ROTARYI, ELSET=hood_rotary
*ROTARY INERTIA, ELSET=hood_rotary
1.e-6,1.e-6,1.e-6
*nset,nset=retained_hood,unsorted
*nset,nset=retained_all
retained_hood,
*End Part
**------------------------------------------------
**
** PART = Rear axle
**
*Part, name=Rear_axle
*Node
********************REAR SPINDLE COUPLING NODES
********************LEFT SIDE
********************RIGHT SIDE
*************************************************
*********************************************************
***reference nodes for rear-axle-driveshaft
*********************************************************
***reference nodes for rear-axle-pent-diff-right coupling
***reference nodes for rear-axle-diff-right coupling
**********************************************************
********************************************************
**reference node for rear-brake-flat-right coupling
**reference node for rear-axle-flat-right coupling
*********************************************************
************************************************************
**reference node for rear-axle-pent-diff-left coupling
**reference node for rear-axle-diff-left coupling
************************************************************
*********************************************************
**reference node for rear-brake-flat-left coupling
**reference node for rear-axle-flat-left coupling
*********************************************************
***Spring nodes
*Element, type=C3D8R
*Element, type=S4R
*Element, type=S3R
*Nset, nset=ALL_NODES
*Elset, elset=REAR-AXLE-UNIVERSAL, generate
*Elset, elset=REAR-AXLE
*Elset, elset=BRAKE-BACK-LEFT, generate
*Elset, elset=BRAKE-BACK-RIGHT, generate
*Elset, elset=EVERYTHING_REAR_AXLE
*Elset, elset=EVERYTHING_ALL
*nset,nset=retained_rear_axle,unsorted
*Elset, elset=REAR-AXLE-FLAT-RIGHT, generate
*Nset, nset=REAR-AXLE-PENT-BRAKE-RIGHT, generate
*Elset, elset=REAR-AXLE-PENT-DIFF-RIGHT, generate
*Elset, elset=REAR-AXLE-DIFF-RIGHT
*Elset, elset=REAR-BRAKE-FLAT-RIGHT, generate
*Elset, elset=REAR-AXLE-FLAT-LEFT, generate
*Nset, nset=REAR-AXLE-PENT-BRAKE-LEFT, generate
*Elset, elset=REAR-AXLE-PENT-DIFF-LEFT, generate
*Elset, elset=REAR-AXLE-DIFF-LEFT
*Elset, elset=REAR-BRAKE-FLAT-LEFT, generate
*Elset, elset=REAR-AXLE-DRIVESHAFT
*Elset, elset=REAR-AXLE-SPINDLE-RIGHT, generate
*Elset, elset=REAR-AXLE-SPINDLE-LEFT, generate
*Elset, elset=_REAR-AXLE-FLAT-RIGHT_SPOS, internal, generate
*Elset, elset=_REAR-AXLE-PENT-DIFF-RIGHT_SNEG, internal, generate
*Elset, elset=_REAR-AXLE-DIFF-RIGHT_SNEG, internal
*Elset, elset=_REAR-BRAKE-FLAT-RIGHT_S1, internal, generate
*Elset, elset=_REAR-AXLE-FLAT-LEFT_SPOS, internal, generate
*Elset, elset=_REAR-AXLE-PENT-DIFF-LEFT_SNEG, internal, generate
*Elset, elset=_REAR-AXLE-DIFF-LEFT_SNEG, internal
*Elset, elset=_REAR-BRAKE-FLAT-LEFT_S1, internal, generate
*Elset, elset=_REAR-AXLE-DRIVESHAFT_SPOS, internal
*Elset, elset=_REAR-AXLE-SPINDLE-RIGHT_S2, internal, generate
*Elset, elset=_REAR-AXLE-SPINDLE-LEFT_S2, internal, generate
*Elset, elset=_REAR-AXLE-UNIVERSAL_SPOS, internal, generate
*nset,nset=rear-axle-pent-brake-right
*nset,nset=rear-axle-pent-brake-left
*Element, type=MASS, elset=REAR-AXLE_MASS
*Mass, elset=REAR-AXLE_MASS
1e-06,
*Element, type=ROTARYI, elset=REAR-AXLE_ROTARY
*RotaryI, elset=REAR-AXLE_ROTARY
*nset,nset=retained_rear_axle_universal
*nset,nset=wheel_spindles
*nset,nset=retained_rear_axle,unsorted
*nset,nset=retained_all
retained_rear_axle,
**
*End Part
**------------------------------------------------
**
** PART = Back_LWheel
**
*Part, name=Back_LWheel
*Node
**
***Ref Node
**
*Element, type=S4R
*Element, type=S3R
*Nset, nset=ALL_NODES
*Elset, elset=OUTER-RIM-BACK-LEFT
*Elset, elset=TIRE-BACK-LEFT, generate
*Elset, elset=INNER-RIM-BACK-LEFT
*Elset, elset=EVERYTHING_WHEEL_BACK_LEFT, generate
*Elset, elset=EVERYTHING_ALL, generate
*Elset, elset=INNER-BACK-LT-RIM-COUP
*nset,nset=retained_wheel_back_left,unsorted
*nset,nset=retained_all
retained_wheel_back_left,
*Elset, elset=_INNER-BACK-LT-RIM-COUP_SPOS, internal
*ELEMENT, TYPE=MASS, ELSET=wheel_back_left_mass
*MASS, ELSET=wheel_back_left_mass
1.e-6,
*ELEMENT, TYPE=ROTARYI, ELSET=wheel_back_left_rotary
*ROTARY INERTIA, ELSET=wheel_back_left_rotary
1.e-6,1.e-6,1.e-6
*End Part
**------------------------------------------------
**
** PART = Back_RWheel
**
*Part, name=Back_RWheel
*Node
**
***Ref Node
**
*Element, type=S4R
*Element, type=S3R
*Nset, nset=ALL_NODES
*Elset, elset=OUTER-RIM-BACK-RIGHT
*Elset, elset=TIRE-BACK-RIGHT, generate
*Elset, elset=INNER-RIM-BACK-RIGHT
*Elset, elset=EVERYTHING_WHEEL_BACK_RIGHT
*Elset, elset=EVERYTHING_ALL
*Elset, elset=INNER-BACK-RT-RIM-COUP
*nset,nset=retained_wheel_back_right,unsorted
*nset,nset=retained_all
retained_wheel_back_right,
*Elset, elset=_INNER-BACK-RT-RIM-COUP_SNEG, internal
*ELEMENT, TYPE=MASS, ELSET=wheel_back_right_mass
*MASS, ELSET=wheel_back_right_mass
1.e-6,
*ELEMENT, TYPE=ROTARYI, ELSET=wheel_back_right_rotary
*ROTARY INERTIA, ELSET=wheel_back_right_rotary
1.e-6,1.e-6,1.e-6
*End Part
**------------------------------------------------
**
** PART = Driveshaft
**
*Part, name=Driveshaft
*Node
*** Ref nodes
***
*Element, type=S4R
*Element, type=S3R
*Nset, nset=ALL_NODES, generate
*Elset, elset=DRIVESHAFT, generate
*Nset, nset=RETAINED_DRIVESHAFT, unsorted
*Nset, nset=RETAINED_ALL
*Elset, elset=EVERYTHING_DRIVESHAFT, generate
*Elset, elset=EVERYTHING_ALL, generate
*Elset, elset=DRIVESHAFT-DIFFERENTIAL
*Elset, elset=DRIVESHAFT-TRANSMISSION
*Elset, elset=_DRIVESHAFT-DIFFERENTIAL_SNEG, internal
*Elset, elset=_DRIVESHAFT-TRANSMISSION_SNEG, internal
*Element, type=MASS, elset=DRIVESHAFT_MASS
*Mass, elset=DRIVESHAFT_MASS
1e-06,
*Element, type=ROTARYI, elset=DRIVESHAFT_ROTARY
*Rotary Inertia, elset=DRIVESHAFT_ROTARY
1e-06, 1e-06, 1e-06, 0., 0., 0.
*End Part
**------------------------------------------------
**
** Part = Engine
**
*Part, name=Engine
*Node
***************************************************
***Beginning of Fan nodes
***END OF FAN NODES
*************************************************
**Reference nodes
**MASS ELEMENT NODES
****************Engine mounting right side
**Reference nodes
***************Engine mounting Rubber left side
*Element, type=C3D8R
*Element, type=S4R
*Element, type=S3R
*Nset, nset=ALL_NODES
*Elset, elset=ENGINE-GEARBOX, generate
*Elset, elset=ENGINE-FRONT, generate
*Elset, elset=ENGINE-OILBOX, generate
*Elset, elset=ENGINE-MNT-REAR, generate
*Elset, elset=ENGINE-MOUNT-LEFT, generate
*Elset, elset=ENGINE-MOUNT-RIGHT, generate
*Elset, elset=ENGINE-MOUNT-TOP-2-LEFT, generate
*Elset, elset=ENGINE-MOUNT-TOP-2-RIGHT, generate
*Elset, elset=ENGINE-MOUNT-TOP-LEFT, generate
*Elset, elset=ENGINE-MOUNT-TOP-RIGHT, generate
*Elset, elset=FAN-CENTER, generate
*Elset, elset=FAN-CENTER-1, generate
*Elset, elset=ENGINE-OUTER, generate
*Elset, elset=GEAR-BOX-CV-JOINT, generate
*Elset, elset=ACCELEROMETER-ENGINE-TOP
*Elset, elset=ACCELEROMETER-ENGINE-BOTTOM
*Nset, nset=ENGINE-CV-JOINT
*Nset, nset=REAR-ENGINE-CV-JOINT
*ELEMENT, TYPE=S4R, ELSET=FAN-CENTER
*ELEMENT, TYPE=S4R, ELSET=FAN-CENTER-1
*ELEMENT, TYPE=B31, ELSET=FAN
*ELEMENT, TYPE=B31, ELSET=OIL-PAN-BEAMS
*Elset, elset=EVERYTHING_ENGINE
*Elset, elset=EVERYTHING_ALL
 Fan-Center-1, Fan-Center
*Nset, nset=NODESET-44
*Nset, nset=NODESET-45
*Elset, elset=_ACCELEROMETER-ENGINE-TOP_S1, internal
*Elset, elset=_ACCELEROMETER-ENGINE-BOTTOM_S1, internal
*Elset, elset=_ENGINE-MNT-REAR_SPOS, internal, generate
*Elset, elset=_ENGINE-MOUNT-TOP-LEFT_SPOS, internal, generate
*Elset, elset=_ENGINE-MOUNT-TOP-RIGHT_SPOS, internal, generate
*Elset, elset=_GEAR-BOX-CV-JOINT_SPOS, internal, generate
*Element, type=MASS, elset=TR_ENGINE_MASS
*Mass, elset=TR_ENGINE_MASS
1e-06,
*Element, type=ROTARYI, elset=TR_ENGINE_ROTARY
*RotaryI, elset=TR_ENGINE_ROTARY
*End Part
**------------------------------------------------
**
** Part = Leaf_springs
**
*Part, name=Leaf_springs
*Node
*Element, type=B31
*Nset, nset=ALL_NODES
*Elset, elset=REAR_SUSP_LEAF_SPRINGS
*Nset, nset=BEAM_NODES
*Elset, elset=EVERYTHING_REAR_SUSP_LEAF_SPRINGS
*BEAM GENERAL SECTION, ELSET=REAR_SUSP_LEAF_SPRINGS, DENSITY=3.5765e-009, rotary inertia=isotropic
 2000.0000, 104200.0000, 0.0000, 1070000.0000, 334000.0000,
 0,1,0
 2.1e5,80769.2308
*End Part
**------------------------------------------------
**
** PART = Front_LWheel
**
*Part, name=Front_LWheel
*Node
**
***Ref Node
**
**
*Element, type=S4R
*Element, type=S3R
*Nset, nset=ALL_NODES
*Elset, elset=OUTER-RIM-FRONT-LEFT
*Elset, elset=TIRE-FRONT-LEFT, generate
*Elset, elset=INNER-RIM-FRONT-LEFT
*Elset, elset=EVERYTHING_WHEEL_FRONT_LEFT, generate
*Elset, elset=EVERYTHING_ALL, generate
*Elset, elset=INNER-FRONT-LT-RIM-COUP
*nset,nset=retained_wheel_front_left,unsorted
*nset,nset=retained_all
retained_wheel_front_left,
*Elset, elset=_INNER-FRONT-LT-RIM-COUP_SPOS, internal
*ELEMENT, TYPE=MASS, ELSET=wheel_front_left_mass
*MASS, ELSET=wheel_front_left_mass
1.e-6,
*ELEMENT, TYPE=ROTARYI, ELSET=wheel_front_left_rotary
*ROTARY INERTIA, ELSET=wheel_front_left_rotary
1.e-6,1.e-6,1.e-6
*End Part
**------------------------------------------------
**
** Part = Brake_left
**
*Part, name=Brake_left
*Node
***Ref node
***Spring node
*Element, type=C3D8R
*Element, type=S4R
*Element, type=S3R
*Nset, nset=ALL_NODES
*Elset, elset=BRAKE_FRONT_LEFT_DISC, generate
*Elset, elset=BRAKE_FRONT_LEFT_HUB_CALIPER, generate
*Elset, elset=BRAKE_FRONT_LEFT_ACCELEROM
*Elset, elset=BRAKE_FRONT_LEFT
*Nset, nset=RB_REFNODES_ALL
*element,type=mass,elset=brake_front_left_mass_lump
*mass,elset=brake_front_left_mass_lump
6.7397927E-02,
*element,type=rotaryi,elset=brake_front_left_rota_lump
*rotary inertia,elset=brake_front_left_rota_lump
385.1161,625.8243,398.8501,7.345737,12.91839,12.09473
**
*ELEMENT, TYPE=MASS, ELSET=brake_front_left_mass
*MASS, ELSET=brake_front_left_mass
1.e-6,
*ELEMENT, TYPE=ROTARYI, ELSET=brake_front_left_rotary
*ROTARY INERTIA, ELSET=brake_front_left_rotary
1.e-6,1.e-6,1.e-6
*Elset, elset=EVERYTHING_BRAKE_LEFT
brake_front_left_mass_lump,brake_front_left_rota_lump
*End Part
**------------------------------------------------
**
** PART = Left_LowerSusp
**
*Part, name=Left_LowerSusp
*Node
*** Ref nodes
*Element, type=S4R
*Element, type=S3R
*Nset, nset=ALL_NODES
*Elset, elset=LOWER_ARM_LEFT
*Elset, elset=LOWER_ARM_LEFT_HOLE_FRONT
*Elset, elset=LOWER_ARM_LEFT_HOLE_BACK
*Nset, nset=RETAINED_LOWER_ARM_LEFT
*Nset, nset=RETAINED_ALL
*Elset, elset=LOWER_ARM_LEFT_TIP
*Elset, elset=EVERYTHING_SUSP_LOWER_ARM_LEFT, generate
*Elset, elset=EVERYTHING_ALL, generate
*Nset, nset=LOWER_ARM_LEFT_STRUT
*Elset, elset=_LOWER_ARM_LEFT_HOLE_FRONT_SPOS, internal
*Elset, elset=_LOWER_ARM_LEFT_HOLE_BACK_SPOS, internal
*Elset, elset=_LOWER_ARM_LEFT_TIP_SPOS, internal
*ELEMENT, TYPE=MASS, ELSET=lower_arm_left_mass
*MASS, ELSET=lower_arm_left_mass
1.e-6,
*ELEMENT, TYPE=ROTARYI, ELSET=lower_arm_left_rotary
*ROTARY INERTIA, ELSET=lower_arm_left_rotary
1.e-6,1.e-6,1.e-6
**--------------------------------------------------------------
*nset,nset=retained_lower_arm_left,unsorted
*nset,nset=retained_all
retained_lower_arm_left,
*End Part
**------------------------------------------------
**
** PART = Left_UpperSusp
**
*Part, name=Left_UpperSusp
*Node
**
***Ref Node
**
*Element, type=S4R
*Element, type=S3R
*Element, type=S3
*Nset, nset=ALL_NODES, generate
*Elset, elset=UPPER_ARM_LEFT
*Elset, elset=UPPER_ARM_LEFT_HOLE_FRONT
*Elset, elset=UPPER_ARM_LEFT_HOLE_BACK
*Elset, elset=UPPER_ARM_LEFT_TIP
*Elset, elset=EVERYTHING_SUSP_UPPER_ARM_LEFT
*Elset, elset=EVERYTHING_ALL
*Elset, elset=_UPPER_ARM_LEFT_HOLE_FRONT_SPOS, internal
*Elset, elset=_UPPER_ARM_LEFT_HOLE_BACK_SPOS, internal
*Elset, elset=_UPPER_ARM_LEFT_TIP_SPOS, internal
*ELEMENT, TYPE=MASS, ELSET=upper_arm_left_mass
**
*MASS, ELSET=upper_arm_left_mass
1.e-6,
*ELEMENT, TYPE=ROTARYI, ELSET=upper_arm_left_rotary
*ROTARY INERTIA, ELSET=upper_arm_left_rotary
1.e-6,1.e-6,1.e-6
*nset,nset=retained_upper_arm_left,unsorted
*nset,nset=retained_all
retained_upper_arm_left,
*End Part
**------------------------------------------------
**
** PART = Front_RWheel
**
*Part, name=Front_RWheel
*Node
**
***Ref Node
**
**
*Element, type=S4R
*Element, type=S3R
*Nset, nset=ALL_NODES
*Elset, elset=OUTER-RIM-FRONT-RIGHT
*Elset, elset=TIRE-FRONT-RIGHT, generate
*Elset, elset=INNER-RIM-FRONT-RIGHT
*Elset, elset=EVERYTHING_WHEEL_FRONT_RIGHT
*Elset, elset=EVERYTHING_ALL
*Elset, elset=INNER-FRONT-RT-RIM-COUP
*nset,nset=retained_wheel_front_right,unsorted
*nset,nset=retained_all
retained_wheel_front_right,
*Elset, elset=_INNER-FRONT-RT-RIM-COUP_SNEG, internal
*ELEMENT, TYPE=MASS, ELSET=wheel_front_right_mass
*MASS, ELSET=wheel_front_right_mass
1.E-6,
*ELEMENT, TYPE=ROTARYI, ELSET=wheel_front_right_rotary
*ROTARY INERTIA, ELSET=wheel_front_right_rotary
1.E-6,1.E-6,1.E-6
*End Part
**------------------------------------------------
**
** Brake right
**
*Part, name=Brake_right
*Node
***Ref node
***Spring node
*Element, type=C3D8R
*Element, type=S4R
*Element, type=S3R
*Nset, nset=ALL_NODES
*Elset, elset=BRAKE_FRONT_RIGHT_DISC, generate
*Elset, elset=BRAKE_FRONT_RIGHT_HUB_CALIPER, generate
*Elset, elset=BRAKE_FRONT_RIGHT_ACCELEROM
*Elset, elset=BRAKE_FRONT_RIGHT
*Nset, nset=RB_REFNODES_ALL
*element,type=mass,elset=brake_front_right_mass_lump
*mass,elset=brake_front_right_mass_lump
6.7397931E-02,
*element,type=rotaryi,elset=brake_front_right_rota_lump
*rotary inertia,elset=brake_front_right_rota_lump
385.1163,625.8245,398.8501,7.345740,12.91825,12.09473
*ELEMENT, TYPE=MASS, ELSET=brake_front_right_mass
*MASS, ELSET=brake_front_right_mass
1.e-6
*ELEMENT, TYPE=ROTARYI, ELSET=brake_front_right_rotary
*ROTARY INERTIA, ELSET=brake_front_right_rotary
1.e-6,1.e-6,1.e-6
*elset, elset=everything_brake_right
brake_front_right_mass_lump,brake_front_right_rota_lump
*End Part
**------------------------------------------------
**
** PART = Right_LowerSusp
**
*Part, name=Right_LowerSusp
*Node
**
***Ref Node
**
*Element, type=S4R
*Element, type=S3R
*Nset, nset=ALL_NODES, generate
*Elset, elset=LOWER_ARM_RIGHT
*Elset, elset=LOWER_ARM_RIGHT_HOLE_FRONT
*Elset, elset=LOWER_ARM_RIGHT_HOLE_BACK
*Elset, elset=LOWER_ARM_RIGHT_TIP
*Elset, elset=EVERYTHING_SUSP_LOWER_ARM_RIGHT, generate
*Elset, elset=EVERYTHING_ALL, generate
*Nset, nset=LOWER_ARM_RIGHT_STRUT
*nset,nset=retained_lower_arm_right,unsorted
*nset,nset=retained_all
retained_lower_arm_right,
*Elset, elset=_LOWER_ARM_RIGHT_HOLE_FRONT_SPOS, internal
*Elset, elset=_LOWER_ARM_RIGHT_HOLE_BACK_SPOS, internal
*Elset, elset=_LOWER_ARM_RIGHT_TIP_SPOS, internal
*ELEMENT, TYPE=MASS, ELSET=lower_arm_right_mass
*MASS, ELSET=lower_arm_right_mass
1e-6,
*ELEMENT, TYPE=ROTARYI, ELSET=lower_arm_right_rotary
*ROTARY INERTIA, ELSET=lower_arm_right_rotary
1e-6,1e-6,1e-6
*End Part
**------------------------------------------------
**
** PART = Right_UpperSusp
**
*Part, name=Right_UpperSusp
*Node
**
***Ref Node
**
*Element, type=S4R
*Element, type=S3R
*Element, type=S3
*Nset, nset=ALL_NODES, generate
*Elset, elset=UPPER_ARM_RIGHT
*Elset, elset=UPPER_ARM_RIGHT_HOLE_FRONT
*Elset, elset=UPPER_ARM_RIGHT_HOLE_BACK
*Elset, elset=UPPER_ARM_RIGHT_TIP
*Elset, elset=EVERYTHING_SUSP_UPPER_ARM_RIGHT
*Elset, elset=EVERYTHING_ALL
*Elset, elset=_UPPER_ARM_RIGHT_HOLE_FRONT_SPOS, internal
*Elset, elset=_UPPER_ARM_RIGHT_HOLE_BACK_SPOS, internal
*Elset, elset=_UPPER_ARM_RIGHT_TIP_SPOS, internal
*ELEMENT, TYPE=MASS, ELSET=upper_arm_right_mass
*MASS, ELSET=upper_arm_right_mass
1.e-6,
*ELEMENT, TYPE=ROTARYI, ELSET=upper_arm_right_rotary
*ROTARY INERTIA, ELSET=upper_arm_right_rotary
1.e-6,1.e-6,1.e-6
*nset,nset=retained_upper_arm_right,unsorted
*nset,nset=retained_all
retained_upper_arm_right,
*End Part
**------------------------------------------------
**
** Part = Steering Rod
**
**------------------------------------------------
**
** PART = LeftTieRod
**
*Part, name=LeftTieRod
*Node
*Element, type=B31
*Nset, nset=ALL_NODES
*Elset, elset=LEFT_TIE_RODS
*Elset, elset=EVERYTHING_LEFT_TIE_RODS
*BEAM GENERAL SECTION, ELSET=LEFT_TIE_rods, DENSITY=7.8900e-009,rotary inertia=isotropic
  452.4000, 16290.0000,0.0000, 16290.0000, 32570.0000,
  210000.0000, 80769.2308
*elset,elset=EVERYTHING_LEFT_TIE_RODS
LEFT_TIE_RODS,
*End Part
**------------------------------------------------
**
** PART = RightTieRod
**
*Part, name=RightTieRod
*Node
*Element, type=B31
*Nset, nset=ALL_NODES
*Elset, elset=RIGHT_TIE_RODS
*Elset, elset=EVERYTHING_RIGHT_TIE_RODS
*BEAM GENERAL SECTION, ELSET=RIGHT_TIE_RODS, DENSITY=7.8900e-009,rotary inertia=isotropic
  452.4000, 16290.0000, 0.0000, 16290.0000, 32570.0000,
  210000.0000, 80769.2308
*elset,elset=EVERYTHING_RIGHT_TIE_RODS
RIGHT_TIE_RODS,
*End Part
**------------------------------------------------
**
** PART = RackRod
**
*Part, name=RackRod
*Node
*Element, type=B31
*Nset, nset=ALL_NODES
*Elset, elset=RACK_RODS
*Elset, elset=EVERYTHING_RACK_RODS
*BEAM GENERAL SECTION, ELSET=RACK_RODS, DENSITY=7.8900e-009,rotary inertia=isotropic
  452.4000, 16290.0000, 0.0000, 16290.0000, 32570.0000,
  210000.0000, 80769.2308
*elset,elset=EVERYTHING_RACK_RODS
RACK_RODS,
*End Part
**------------------------------------------------
**
** PART = Stabilizer
**
*Part, name=Stabilizer
*Node
*ELEMENT, TYPE=B31, ELSET=stabilizer_bar
*Nset, nset=ALL_NODES, generate
*Elset, elset=STABILIZER_BAR, generate
*Nset, nset=RETAINED_STABILIZER_BAR
*Nset, nset=BEAM_NODES, generate
*BEAM GENERAL SECTION, ELSET=stabilizer_bar, DENSITY=7.8900e-009,rotary inertia=isotropic
  452.4000, 16290.0000, 0.0000, 16290.0000, 32570.0000,
  210000.0000, 80769.2308
*Elset, elset=EVERYTHING_STABILIZER, generate
*End Part
**------------------------------------------------
**************************************************************
**                   TIRE UELS                              **
**************************************************************
**************************************************************
**
** PART = tire_front_lt_uel
**
*Part, name=tire_front_lt_uel
*Node
**990804
*user element,nodes=1,type=u3,properties=5,i properties=3,
coordinates=3,variables=12
*element, type=u3, elset=tire_front_lt
*uel property, elset=tire_front_lt
<tire_rad_stiff>,<tire_front_lt_ref_rad>,<bump_length>,<bump_height>,<x_bump_start>,<bumps_in_phase>,<lat_force_include>,<self_align_include>
*End Part
**------------------------------------------------
**
** PART = tire_front_rt_uel
**
*Part, name=tire_front_rt_uel
*Node
**990806
*user element,nodes=1,type=u3,properties=5,i properties=3,
coordinates=3,variables=12
*element, type=u3, elset=tire_front_rt
*uel property, elset=tire_front_rt
<tire_rad_stiff>,<tire_front_rt_ref_rad>,<bump_length>,<bump_height>,<x_bump_start>,<bumps_in_phase>,<lat_force_include>,<self_align_include>
*End Part
**------------------------------------------------
**
** PART = tire_rear_lt_uel
**
*Part, name=tire_rear_lt_uel
*Node
**990808
*user element,nodes=1,type=u3,properties=5,i properties=3,
coordinates=3,variables=12
*element, type=u3, elset=tire_rear_lt
*uel property, elset=tire_rear_lt
<tire_rad_stiff>,<tire_rear_lt_ref_rad>,<bump_length>,<bump_height>,<x_bump_start>,<bumps_in_phase>,<lat_force_include>,<self_align_include>
*End Part
**------------------------------------------------
**
** PART = tire_rear_rt_uel
**
*Part, name=tire_rear_rt_uel
*Node
**990809
*user element,nodes=1,type=u3,properties=5,i properties=3,
coordinates=3,variables=12
*element, type=u3, elset=tire_rear_rt
*uel property, elset=tire_rear_rt
<tire_rad_stiff>,<tire_rear_rt_ref_rad>,<bump_length>,<bump_height>,<x_bump_start>,<bumps_in_phase>,<lat_force_include>,<self_align_include>
*End Part
**------------------------------------------------
**
** PART = Road
**
*Part, name=Road
*Node, nset=RIGID-ROAD
******
******
******
*ELEMENT,TYPE=M3D4,ELSET=roadshell
*ELGEN, ELSET=roadshell
*End Part
**------------------------------------------------
**------------------------------------------------
**------------------------------------------------
**
** ASSEMBLY
**
*Assembly, name=Assembly
*Instance, name=Bed-1, part=Bed
*End Instance
*Instance, name=Chassis-1, part=Chassis
*End Instance
*Instance, name=Fuel_Tank-1, part=Fuel_Tank
*End Instance
*Instance, name=Bumper-1, part=Bumper
*End Instance
*Instance, name=Cabin-1, part=Cabin
*End Instance
*Instance, name=Seat-1, part=Seat
*End Instance
*Instance, name=Left_Door-1, part=Left_Door
*End Instance
*Instance, name=Right_Door-1, part=Right_Door
*End Instance
*Instance, name=Hood-1, part=Hood
*End Instance
*Instance, name=Rear_axle-1, part=Rear_axle
*End Instance
*Instance, name=Back_LWheel-1, part=Back_LWheel
*End Instance
*Instance, name=Back_RWheel-1, part=Back_RWheel
*End Instance
*Instance, name=Driveshaft-1, part=Driveshaft
*End Instance
*Instance, name=Engine-1, part=Engine
*End Instance
*Instance, name=Leaf_springs-1, part=Leaf_springs
*End Instance
*Instance, name=Front_LWheel-1, part=Front_LWheel
*End Instance
*Instance, name=Brake_left-1, part=Brake_left
*End Instance
*Instance, name=Left_LowerSusp-1, part=Left_LowerSusp
*End Instance
*Instance, name=Left_UpperSusp-1, part=Left_UpperSusp
*End Instance
*Instance, name=Front_RWheel-1, part=Front_RWheel
*End Instance
*Instance, name=Brake_right-1, part=Brake_right
*End Instance
*Instance, name=Right_LowerSusp-1, part=Right_LowerSusp
*End Instance
*Instance, name=Right_UpperSusp-1, part=Right_UpperSusp
*End Instance
*Instance, name=LeftTieRod-1, part=LeftTieRod
*End Instance
*Instance, name=RightTieRod-1, part=RightTieRod
*End Instance
*Instance, name=RackRod-1, part=RackRod
*End Instance
*Instance, name=Stabilizer-1, part=Stabilizer
*End Instance
*Instance, name=tire_front_lt_uel-1, part=tire_front_lt_uel
*End Instance
*Instance, name=tire_front_rt_uel-1, part=tire_front_rt_uel
*End Instance
*Instance, name=tire_rear_lt_uel-1, part=tire_rear_lt_uel
*End Instance
*Instance, name=tire_rear_rt_uel-1, part=tire_rear_rt_uel
*End Instance
*Instance, name=Road-1, part=Road
*End Instance
**------------------------------------------------
**------------------------------------------------
*Orientation, Name=Ori1, System=Rectangular
**------------------------------------------------
**------------------------------------------------
***Center of mass of the bed
*Node
**********
*Display Body, INSTANCE=Bed-1
**retained nodes of the bed
*Node
**1900762
**1901143
**161057
**161436
**191234
**191200
**1901286
**161568
*******
*Nset, nset=bed_all, generate
*******
** Bed center of mass
*Element, Type=MASS, ELSET=bed_center_of_mass
*MASS, ELSET=bed_center_of_mass
0.3043972,
*Element, Type=ROTARYI, ELSET=bed_rotary_center_of_mass
*ROTARY INERTIA, ELSET=bed_rotary_center_of_mass
160387.5, 260236.4, 393366.8
*******
** Bed retained nodes
*Element, Type=MASS, ELSET=bed_retained_nodes_mass
*MASS, ELSET=bed_retained_nodes_mass
1.e-5
*Element, Type=ROTARYI, ELSET=bed_rotary_retained_nodes
*ROTARY INERTIA, ELSET=bed_rotary_retained_nodes
16, 26, 39
*******
*Element, Type=CONN3D2, ELSET=bed_db_retained_nodes
**
*Connector section, ELSET=bed_db_retained_nodes, Behavior=sbehavior
cardan, cartesian
Ori1
*Element, Type=CONN3D2, ELSET=bed_db_retained_nodes1
*Connector section, ELSET=bed_db_retained_nodes1, Behavior=sbehavior
cardan, cartesian
Ori1
**------------------------------------------------
**------------------------------------------------
***Center of mass of the chassis
*Node
**********
*Display Body, INSTANCE=Chassis-1
**retained nodes of the chassis
*Node
**211380
**211475
**211794
**212195
**258003
**258521
**101837
**101832
**94467
**94462
**903456
**903457
**903464
**903462
**971498
**971495
**1207008
**1207015
**4775462
**9000016
**9000014
**1105030
**224109
**281661
**225059
**281576
**2900762
**2901143
**261057
**261436
**291234
**291200
**2901286
**261568
**1821032
**1821031
**1821016
**1821015
**9200031
**9200032
**9200033
**9200034
*******
*Nset, nset=chassis_all, generate
*Nset, nset=retained_chassis, generate
*******
** Chassis center of mass
*Element, Type=MASS, ELSET=chassis_center_of_mass
*MASS, ELSET=chassis_center_of_mass
0.1395620,
*Element, Type=ROTARYI, ELSET=chassis_rotary_center_of_mass
*ROTARY INERTIA, ELSET=chassis_rotary_center_of_mass
31154.84, 258693.8, 286045.2
*******
** Chassis retained nodes
*Element, Type=MASS, ELSET=chassis_retained_nodes_mass
*MASS, ELSET=chassis_retained_nodes_mass
1.e-5
*Element, Type=ROTARYI, ELSET=chassis_rotary_retained_nodes
*ROTARY INERTIA, ELSET=chassis_rotary_retained_nodes
3, 25, 28
*******
*Element, Type=CONN3D2, ELSET=chassis_db_retained_nodes
**
*Connector section, ELSET=chassis_db_retained_nodes
beam
*Element, Type=CONN3D2, ELSET=chassis_db_retained_nodes1
*Connector section, ELSET=chassis_db_retained_nodes1, Behavior=sbehavior
cardan, cartesian
Ori1
**------------------------------------------------
**------------------------------------------------
**********
***Center of mass of the Fuel Tank
*Node
*Display Body, INSTANCE=Fuel_Tank-1
**retained nodes of the Fuel Tank
*Node
**9190031
**9190032
**9190033
**9190034
*******
*Nset, nset=fuel_tank_all, generate
*******
** Fuel_Tank center of mass
*Element, Type=MASS, ELSET=Fuel_Tank_center_of_mass
*Mass, ELSET=Fuel_Tank_center_of_mass
0.065097344
*Element, Type=ROTARYI, ELSET=Fuel_Tank_rotary_center_of_mass
*ROTARY INERTIA, ELSET=Fuel_Tank_rotary_center_of_mass
2290.500, 13877.05, 14259.24
*******
** Fuel_Tank retained nodes
*Element, Type=MASS, ELSET=Fuel_Tank_retained_nodes_mass
*MASS, ELSET=Fuel_Tank_retained_nodes_mass
1.e-5
*Element, Type=ROTARYI, ELSET=Fuel_Tank_rotary_retained_nodes
*ROTARY INERTIA, ELSET=Fuel_Tank_rotary_retained_nodes
0.2, 1.3, 1.4
*******
*Element, Type=CONN3D2, ELSET=Fuel_Tank_db_retained_nodes
*Connector section, ELSET=Fuel_Tank_db_retained_nodes, Behavior=sbehavior
cartesian, cardan
Ori1
**------------------------------------------------
**------------------------------------------------
**********
***Center of mass of the bumper
*Node
*Display Body, INSTANCE=Bumper-1
**retained nodes of the bumper
*Node
**111380
**111794
**111475
**112195
*******
*Nset, nset=bumper_all, generate
*******
** Bumper center of mass
*Element, Type=MASS, ELSET=bumper_center_of_mass
*Mass, ELSET=bumper_center_of_mass
0.020261725
*Element, Type=ROTARYI, ELSET=bumper_rotary_center_of_mass
*ROTARY INERTIA, ELSET=bumper_rotary_center_of_mass
6990.777, 353.7216, 7112.266
*******
** Bumper retained nodes
*Element, Type=MASS, ELSET=Bumper_retained_nodes_mass
*MASS, ELSET=Bumper_retained_nodes_mass
1.e-5
*Element, Type=ROTARYI, ELSET=Bumper_rotary_retained_nodes
*ROTARY INERTIA, ELSET=Bumper_rotary_retained_nodes
0.6, 0.03, 0.7
*******
*Element, Type=CONN3D2, ELSET=bumper_db_retained_nodes
*Connector section, ELSET=bumper_db_retained_nodes
beam
*Element, Type=CONN3D2, ELSET=bumper_db_retained_nodes1
*Connector section, ELSET=bumper_db_retained_nodes1, Behavior=sbehavior
cardan, cartesian
Ori1
**------------------------------------------------
**------------------------------------------------
**********
***Center of mass of the cabin
*Node
*Display Body, INSTANCE=Cabin-1
**retained nodes of the engine
*Node
**181576
**124109
**181661
**125059
**158003
**158521
**9000011
**9000009
**1800291
**9000005
**9000007
**1800142
**284775
**284140
**1810218
**128552
**128064
**128052
**128564
**1990460
**3990460
*******
*Nset, nset=cabin_all, generate
*******
** Cabin center of mass
*Element, Type=MASS, ELSET=cabin_center_of_mass
*Mass, ELSET=cabin_center_of_mass
0.2828125
*Element, Type=ROTARYI, ELSET=cabin_rotary_center_of_mass
*ROTARY INERTIA, ELSET=cabin_rotary_center_of_mass
117590.7, 279841.8, 316385.6
*******
** Cabin retained nodes
*Element, Type=MASS, ELSET=Cabin_retained_nodes_mass
**40100101, 39900220
*MASS, ELSET=Cabin_retained_nodes_mass
1.e-5
*Element, Type=ROTARYI, ELSET=Cabin_rotary_retained_nodes
**50100101, 39900220
*ROTARY INERTIA, ELSET=Cabin_rotary_retained_nodes
11, 27, 31
*******
*Element, Type=CONN3D2, ELSET=cabin_db_retained_nodes
*Connector section, ELSET=cabin_db_retained_nodes
beam
**
*Element, Type=CONN3D2, ELSET=cabin_db_retained_nodes_overconstrained
*Connector section, ELSET=cabin_db_retained_nodes_overconstrained, Behavior=sbehavior
cardan, cartesian
Ori1,
*Nset, nset=retained_cabin_cg
**------------------------------------------------
**------------------------------------------------
**********
***Center of mass of the seat
*Node
*Display Body, INSTANCE=Seat-1
**retained nodes of the seat
*Node
**8064
**8052
**8552
**8564
*******
*Nset, nset=seat_all, generate
*******
** Seat center of mass
*Element, Type=MASS, ELSET=seat_center_of_mass
*Mass, ELSET=seat_center_of_mass
0.035354510
*Element, Type=ROTARYI, ELSET=seat_rotary_center_of_mass
*ROTARY INERTIA, ELSET=seat_rotary_center_of_mass
8813.443, 3122.045, 8512.036
*******
** Seat retained nodes
*Element, Type=MASS, ELSET=Seat_retained_nodes_mass
*MASS, ELSET=Seat_retained_nodes_mass
1.e-5
*Element, Type=ROTARYI, ELSET=Seat_rotary_retained_nodes
*ROTARY INERTIA, ELSET=Seat_rotary_retained_nodes
0.8, 0.3, 0.8
*******
*Element, Type=CONN3D2, ELSET=seat_db_retained_nodes
*Connector section, ELSET=seat_db_retained_nodes
beam
**------------------------------------------------
**------------------------------------------------
**********
***Center of mass of the left door
*Node
*Display Body, INSTANCE=Left_Door-1
**retained nodes of the left door
*Node
**9000010
**9000012
**1800215
*******
*Nset, nset=left_door_all, generate
*******
** left_door center of mass
*Element, Type=MASS, ELSET=left_door_center_of_mass
*Mass, ELSET=left_door_center_of_mass
0.028878174
*Element, Type=ROTARYI, ELSET=left_door_rotary_center_of_mass
*ROTARY INERTIA, ELSET=left_door_rotary_center_of_mass
3347.423, 7451.323, 4373.396
*******
** left_door retained nodes
*Element, Type=MASS, ELSET=left_door_retained_nodes_mass
*MASS, ELSET=left_door_retained_nodes_mass
1.e-5
*Element, Type=ROTARYI, ELSET=left_door_rotary_retained_nodes
*ROTARY INERTIA, ELSET=left_door_rotary_retained_nodes
0.3, 0.7, 0.4
*******
*Element, Type=CONN3D2, ELSET=left_door_db_retained_nodes
*Connector section, ELSET=left_door_db_retained_nodes
beam
**------------------------------------------------
**------------------------------------------------
**********
***Center of mass of the right door
*Node
*Display Body, INSTANCE=Right_Door-1
**retained nodes of the right door
*Node
**9000006
**9000008
**1800066
*******
*Nset, nset=right_door_all, generate
*******
** right_door center of mass
*Element, Type=MASS, ELSET=right_door_center_of_mass
*Mass, ELSET=right_door_center_of_mass
0.028884241
*Element, Type=ROTARYI, ELSET=right_door_rotary_center_of_mass
*ROTARY INERTIA, ELSET=right_door_rotary_center_of_mass
3349.440, 7455.849, 4373.558
*******
** right_door retained nodes
*Element, Type=MASS, ELSET=right_door_retained_nodes_mass
*MASS, ELSET=right_door_retained_nodes_mass
1.e-5
*Element, Type=ROTARYI, ELSET=right_door_rotary_retained_nodes
*ROTARY INERTIA, ELSET=right_door_rotary_retained_nodes
0.3, 0.7, 0.4
*******
*Element, Type=CONN3D2, ELSET=right_door_db_retained_nodes
*Connector section, ELSET=right_door_db_retained_nodes
beam
**------------------------------------------------
**------------------------------------------------
**********
***Center of mass of the hood
*Node
*Display Body, INSTANCE=Hood-1
**retained nodes of the hood
*Node
**184775,
**184140
**2810218,
*******
*Nset, nset=hood_all, generate
*******
** hood center of mass
*Element, Type=MASS, ELSET=hood_center_of_mass
*Mass, ELSET=hood_center_of_mass
0.020261725
*Element, Type=ROTARYI, ELSET=hood_rotary_center_of_mass
*ROTARY INERTIA, ELSET=hood_rotary_center_of_mass
4882.576, 2482.104, 7205.477
*******
** hood retained nodes
*Element, Type=MASS, ELSET=hood_retained_nodes_mass
*MASS, ELSET=hood_retained_nodes_mass
1.e-5
*Element, Type=ROTARYI, ELSET=hood_rotary_retained_nodes
*ROTARY INERTIA, ELSET=hood_rotary_retained_nodes
0.4, 0.2, 0.7
**73.86, 398.50, 435.25
*******
*Element, Type=CONN3D2, ELSET=hood_db_retained_nodes
*Connector section, ELSET=hood_db_retained_nodes, Behavior=sbehavior
cardan, cartesian
Ori1
**********
***Center of mass of the rear axle
*Node
**********
*Display Body, INSTANCE=Rear_axle-1
**retained nodes of the rear axle
*Node
**983102
**990808
**990809
*******
*Nset, nset=rear_axle_all, generate
*******
** Rear_axle center of mass
*Element, Type=MASS, ELSET=rear-axle_center_of_mass
*MASS, ELSET=rear-axle_center_of_mass
0.079363803
*Element, Type=ROTARYI, ELSET=rear-axle_rotary_center_of_mass
*ROTARY INERTIA, ELSET=rear-axle_rotary_center_of_mass
30318.77, 771.8673, 30444.60
*******
** Rear_axle retained nodes
*Element, Type=MASS, ELSET=Rear_axle_retained_nodes_mass
*MASS, ELSET=Rear_axle_retained_nodes_mass
1.e-5
**
**
**
********************************************
** INTRODUCE THIS ROTARYI element TO REMOVE
** ZERO PIVOT MESSAGES IN IMPACT SOLVER PASSES
**
*Element, Type=ROTARYI, ELSET=Remove_ZeroPivots
*ROTARY INERTIA, ELSET=Remove_ZeroPivots
1.e-10,1.e-10,1.e-10
**
** ROTARYI element ABOVE INTRODUCED TO REMOVE
** ZERO PIVOTS
** ***********************************************
**
**
**
*Element, Type=ROTARYI, ELSET=Rear_axle_rotary_retained_nodes
*ROTARY INERTIA, ELSET=Rear_axle_rotary_retained_nodes
3, 0.07, 3
*******
*Element, Type=CONN3D2, ELSET=rear-axle_db_retained_nodes
*Connector section, ELSET=rear-axle_db_retained_nodes, Behavior=sbehavior
cardan, cartesian
Ori1
*Element, Type=CONN3D2, ELSET=rear-axle_db_retained_nodes1
*Connector section, ELSET=rear-axle_db_retained_nodes1, BEHAVIOR=sbehavior
cardan, cartesian
Ori1,
*Element, Type=CONN3D2, ELSET=rear-axle_db_retained_nodes2
*Connector section, ELSET=rear-axle_db_retained_nodes2
beam
**********
***Center of mass of the back left-wheel
*Node
**********
*Display Body, INSTANCE=Back_LWheel-1
**retained nodes of the back left wheel
*Node
**982012
**902621
**902763
**902465
*******
*Nset, nset=back_lwheel_all, generate
*******
** Back_LWheel center of mass
*Element, Type=MASS, ELSET=back_lwheel_center_of_mass
*Mass, ELSET=back_lwheel_center_of_mass
0.033151059
*Element, Type=ROTARYI, ELSET=back_lwheel_rotary_center_of_mass
*ROTARY INERTIA, ELSET=back_lwheel_rotary_center_of_mass
1477.229, 2566.045, 1477.248
*******
** Back_LWheel retained nodes
*Element, Type=MASS, ELSET=Back_LWheel_retained_nodes_mass
*MASS, ELSET=Back_LWheel_retained_nodes_mass
1.e-5
*Element, Type=ROTARYI, ELSET=Back_LWheel_rotary_retained_nodes
*ROTARY INERTIA, ELSET=Back_LWheel_rotary_retained_nodes
0.1, 0.2, 0.1
*******
*Element, Type=CONN3D2, ELSET=back_lwheel_db_retained_nodes
*Connector section, ELSET=back_lwheel_db_retained_nodes, Behavior=sbehavior
cardan, cartesian
Ori1
**********
***Center of mass of the back right-wheel
*Node
*Display Body, INSTANCE=Back_RWheel-1
**retained nodes of the back right wheel
*Node
**982002
**930249
**930354
**930112,
*******
*Nset, nset=back_rwheel_all, generate
*******
** Back_RWheel center of mass
*Element, Type=MASS, ELSET=back_rwheel_center_of_mass
*Mass, ELSET=back_rwheel_center_of_mass
0.03315106
*Element, Type=ROTARYI, ELSET=back_rwheel_rotary_center_of_mass
*ROTARY INERTIA, ELSET=back_rwheel_rotary_center_of_mass
1477.230, 2566.046, 1477.248
*******
** Back_RWheel retained nodes
*Element, Type=MASS, ELSET=Back_RWheel_retained_nodes_mass
*MASS, ELSET=Back_RWheel_retained_nodes_mass
1.e-5
*Element, Type=ROTARYI, ELSET=Back_RWheel_rotary_retained_nodes
*ROTARY INERTIA, ELSET=Back_RWheel_rotary_retained_nodes
0.1, 0.2, 0.1
*******
*Element, Type=CONN3D2, ELSET=back_rwheel_db_retained_nodes
*Connector section, ELSET=back_rwheel_db_retained_nodes, Behavior=sbehavior
cardan, cartesian
Ori1
**---------------------------------------
*ORIENTATION,NAME=ori_wheels_back
**---------------------------------------
*ELEMENT, TYPE=CONN3D2, ELSET=conn_wheel_spindle_rear_left
*CONNECTOR SECTION, ELSET=conn_wheel_spindle_rear_left, BEHAVIOR=conn_wheel_spindle_back
join,revolute
ori_wheels_back,
**---------------------------------------
*ELEMENT, TYPE=CONN3D2, ELSET=conn_wheel_spindle_rear_right
*CONNECTOR SECTION, ELSET=conn_wheel_spindle_rear_right, BEHAVIOR=conn_wheel_spindle_back
join,revolute
ori_wheels_back,
**---------------------------------------
**********
***Center of mass of the driveshaft
*Node
*Display Body, INSTANCE=Driveshaft-1
**retained nodes of the driveshaft
*Node
**983103
**983101
*******
*Nset, nset=driveshaft_all, generate
*******
** Driveshaft center of mass
*Element, Type=MASS, ELSET=driveshaft_center_of_mass
*Mass, ELSET=driveshaft_center_of_mass
0.035145043
*Element, Type=ROTARYI, ELSET=driveshaft_rotary_center_of_mass
*ROTARY INERTIA, ELSET=driveshaft_rotary_center_of_mass
157.9822, 10378.43, 10323.98
*******
** Driveshaft retained nodes
*Element, Type=MASS, ELSET=Driveshaft_retained_nodes_mass
*MASS, ELSET=Driveshaft_retained_nodes_mass
1.e-5
*Element, Type=ROTARYI, ELSET=Driveshaft_rotary_retained_nodes
*ROTARY INERTIA, ELSET=Driveshaft_rotary_retained_nodes
0.01, 1.0, 1.0
*******
*Element, Type=CONN3D2, ELSET=driveshaft_db_retained_nodes1
*Connector section, ELSET=driveshaft_db_retained_nodes1, Behavior=sbehavior
cardan, cartesian
Ori1
**
**********
***Center of mass of the engine
*Node
*Display Body, INSTANCE=Engine-1
**retained nodes of the engine
*Node
**2105030
**9000015
**9000013
**983100
*******
*Nset, nset=engine_all, generate
*******
** Engine center of mass
*Element, Type=MASS, ELSET=engine_center_of_mass
*Mass, ELSET=engine_center_of_mass
0.3514492
*Element, Type=ROTARYI, ELSET=engine_rotary_center_of_mass
*ROTARY INERTIA, ELSET=engine_rotary_center_of_mass
11656.72, 36067.00, 34907.39
*******
** Engine retained nodes
*Element, Type=MASS, ELSET=Engine_retained_nodes_mass
*MASS, ELSET=Engine_retained_nodes_mass
1.e-5
*Element, Type=ROTARYI, ELSET=Engine_rotary_retained_nodes
*ROTARY INERTIA, ELSET=Engine_rotary_retained_nodes
1, 3, 3
*******
*Element, Type=CONN3D2, ELSET=engine_db_retained_nodes
*Connector section, ELSET=engine_db_retained_nodes
beam
*Element, Type=CONN3D2, ELSET=engine_db_retained_nodes1
*Connector section, ELSET=engine_db_retained_nodes1, Behavior=sbehavior
cardan, cartesian
Ori1
**********
***Center of mass of the front left-wheel
*Node
*Display Body, INSTANCE=Front_LWheel-1
**retained nodes of the front left wheel
*Node
**940177
**940375
**940117
*******
*Nset, nset=front_lwheel_all, generate
*******
** Front_LWheel center of mass
*Element, Type=MASS, ELSET=front_lwheel_center_of_mass
*Mass, ELSET=front_lwheel_center_of_mass
0.033146997
*Element, Type=ROTARYI, ELSET=front_lwheel_rotary_center_of_mass
*ROTARY INERTIA, ELSET=front_lwheel_rotary_center_of_mass
1477.203, 2566.024, 1477.247
*******
** Front_LWheel retained nodes
*Element, Type=MASS, ELSET=Front_LWheel_retained_nodes_mass
*MASS, ELSET=Front_LWheel_retained_nodes_mass
1.e-5
*Element, Type=ROTARYI, ELSET=Front_LWheel_rotary_retained_nodes
*ROTARY INERTIA, ELSET=Front_LWheel_rotary_retained_nodes
0.1, 0.2, 0.1
*Element, Type=CONN3D2, ELSET=front_lwheel_db_retained_nodes
*Connector section, ELSET=front_lwheel_db_retained_nodes, Behavior=sbehavior
cardan, cartesian
Ori1,
**********
***Center of mass of the Brake_left
*Node
*Display Body, INSTANCE=Brake_left-1
**retained nodes of the Brake_left
*Node
**906342
**906340
**3860663
**990804
*******
*Nset, nset=brake_left_all, generate
*******
** Brake_left center of mass
*Element, Type=MASS, ELSET=Brake_left_center_of_mass
*Mass, ELSET=Brake_left_center_of_mass
0.067401927
*Element, Type=ROTARYI, ELSET=Brake_left_rotary_center_of_mass
*ROTARY INERTIA, ELSET=Brake_left_rotary_center_of_mass
385.1970, 625.8971, 398.9089
*******
** Brake_left retained nodes
*Element, Type=MASS, ELSET=Brake_left_retained_nodes_mass
*MASS, ELSET=Brake_left_retained_nodes_mass
1.e-5
*Element, Type=ROTARYI, ELSET=Brake_left_rotary_retained_nodes
*ROTARY INERTIA, ELSET=Brake_left_rotary_retained_nodes
0.03, 0.06, 0.03
*******
*Element, Type=CONN3D2, ELSET=Brake_left_db_retained_nodes
*Connector section, ELSET=Brake_left_db_retained_nodes, Behavior=sbehavior
cartesian, cardan
Ori1
*Elset, elset=probeLWheel
*Element, Type=CONN3D2, ELSET=Brake_left_db_retained_nodes1
*Connector section, ELSET=Brake_left_db_retained_nodes1
beam
**---------------------------------------
*********************************************************
**** connector definitions from the tr_conn_wheels_front.inp file
*********************************************************
*ORIENTATION,NAME=ori_wheels_front
*ELEMENT, TYPE=CONN3D2, ELSET=conn_wheel_spindle_front_left
*CONNECTOR SECTION, ELSET=conn_wheel_spindle_front_left, BEHAVIOR=conn_wheel_spindle_front
join, revolute
ori_wheels_front,
**---------------------------------------
**********
***Center of mass of the Left_LowerSusp
*Node
*Display Body, INSTANCE=Left_LowerSusp-1
**retained nodes of the Left_LowerSusp
*Node
**101834
**101831
**906343
**971496
**101470
*******
*Nset, nset=left_lowersusp_all, generate
*******
** Left_LowerSusp center of mass
*Element, Type=MASS, ELSET=Left_LowerSusp_center_of_mass
*Mass, ELSET=Left_LowerSusp_center_of_mass
0.0078959598
*Element, Type=ROTARYI, ELSET=Left_LowerSusp_rotary_center_of_mass
*ROTARY INERTIA, ELSET=Left_LowerSusp_rotary_center_of_mass
115.0264, 142.2430, 224.0555
*******
** Left_LowerSusp retained nodes
*Element, Type=MASS, ELSET=Left_LowerSusp_retained_nodes_mass
*MASS, ELSET=Left_LowerSusp_retained_nodes_mass
1.e-5
*Element, Type=ROTARYI, ELSET=Left_LowerSusp_rotary_retained_nodes
*ROTARY INERTIA, ELSET=Left_LowerSusp_rotary_retained_nodes
0.01, 0.01, 0.02
*******
*Element, Type=CONN3D2, ELSET=Left_LowerSusp_db_retained_nodes
*Connector section, ELSET=Left_LowerSusp_db_retained_nodes
beam
*Element, Type=CONN3D2, ELSET=Left_LowerSusp_db_retained_nodes1
*Connector section, ELSET=Left_LowerSusp_db_retained_nodes1, Behavior=sbehavior
cardan, cartesian
Ori1
*********************************************************
**** connector definitions from the tr_conn_brake_left.inp file
*********************************************************
**---------------------------------------
*ELEMENT, TYPE=CONN3D2, ELSET=conn_lower_arm_join_left
*CONNECTOR SECTION, ELSET=conn_lower_arm_join_left
join,
**---------------------------------------
**********
***Center of mass of the Left_UpperSusp
*Node
*Display Body, INSTANCE=Left_UpperSusp-1
**retained nodes of the Left_UpperSusp
*Node
**101294
**903454
**906341
*******
*Nset, nset=left_uppersusp_all, generate
*******
** Left_UpperSusp center of mass
*Element, Type=MASS, ELSET=Left_UpperSusp_center_of_mass
*Mass, ELSET=Left_UpperSusp_center_of_mass
0.0028873227
*Element, Type=ROTARYI, ELSET=Left_UpperSusp_rotary_center_of_mass
*ROTARY INERTIA, ELSET=Left_UpperSusp_rotary_center_of_mass
21.24922, 39.77147, 46.89484
*******
** Left_UpperSusp retained nodes
*Element, Type=MASS, ELSET=Left_UpperSusp_retained_nodes_mass
*MASS, ELSET=Left_UpperSusp_retained_nodes_mass
1.e-5
*Element, Type=ROTARYI, ELSET=Left_UpperSusp_rotary_retained_nodes
*ROTARY INERTIA, ELSET=Left_UpperSusp_rotary_retained_nodes
0.002, 0.003, 0.004
*******
*Element, Type=CONN3D2, ELSET=Left_UpperSusp_db_retained_nodes
*Connector section, ELSET=Left_UpperSusp_db_retained_nodes, Behavior=sbehavior
cardan, cartesian
Ori1
*********************************************************
**** connector definitions from the tr_conn_brake_left.inp file
*********************************************************
**---------------------------------------
*ELEMENT, TYPE=CONN3D2, ELSET=conn_upper_arm_join_left
*CONNECTOR SECTION, ELSET=conn_upper_arm_join_left
join,
**---------------------------------------
**********
***Center of mass of the front right-wheel
*Node
*Display Body, INSTANCE=Front_RWheel-1
**retained nodes of the front right wheel
*Node
**960181
**960045
**960305
*******
*Nset, nset=front_rwheel_all, generate
*******
** Front_RWheel center of mass
*Element, Type=MASS, ELSET=front_rwheel_center_of_mass
*Mass, ELSET=front_rwheel_center_of_mass
0.033147002
*Element, Type=ROTARYI, ELSET=front_rwheel_rotary_center_of_mass
*ROTARY INERTIA, ELSET=front_rwheel_rotary_center_of_mass
1477.204, 2566.025, 1477.247
*******
** Front_RWheel retained nodes
*Element, Type=MASS, ELSET=Front_RWheel_retained_nodes_mass
*MASS, ELSET=Front_RWheel_retained_nodes_mass
1.e-5
*Element, Type=ROTARYI, ELSET=Front_RWheel_rotary_retained_nodes
*ROTARY INERTIA, ELSET=Front_RWheel_rotary_retained_nodes
0.1, 0.2, 0.1
*Element, Type=CONN3D2, ELSET=front_rwheel_db_retained_nodes
*Connector section, ELSET=front_rwheel_db_retained_nodes, Behavior=sbehavior
cardan, cartesian
Ori1
**********
***Center of mass of the Brake_right
*Node
*Display Body, INSTANCE=Brake_right-1
**retained nodes of the Brake_right
*Node
**906346
**906344
**3905294
**990806
*******
*Nset, nset=brake_right_all, generate
*******
*Element, Type=MASS, ELSET=Brake_right_center_of_mass
*Mass, ELSET=Brake_right_center_of_mass
0.067401931
*Element, Type=ROTARYI, ELSET=Brake_right_rotary_center_of_mass
*ROTARY INERTIA, ELSET=Brake_right_rotary_center_of_mass
385.1972, 625.8973, 398.9089
*******
** Brake_right retained nodes
*Element, Type=MASS, ELSET=Brake_right_retained_nodes_mass
*MASS, ELSET=Brake_right_retained_nodes_mass
1.e-5
*Element, Type=ROTARYI, ELSET=Brake_right_rotary_retained_nodes
*ROTARY INERTIA, ELSET=Brake_right_rotary_retained_nodes
0.03, 0.06, 0.03
*Element, Type=CONN3D2, ELSET=Brake_right_db_retained_nodes
*Connector section, ELSET=Brake_right_db_retained_nodes, Behavior=sbehavior
cardan, cartesian
Ori1
*Elset, elset=probeRWheel
*Element, Type=CONN3D2, ELSET=Brake_right_db_retained_nodes1
*Connector section, ELSET=Brake_right_db_retained_nodes1
Beam
**------------------------------------------------
*********************************************************
**** connector definitions from the tr_conn_wheels_front.inp file
*********************************************************
**---------------------------------------
*ELEMENT, TYPE=CONN3D2, ELSET=conn_wheel_spindle_front_right
*CONNECTOR SECTION, ELSET=conn_wheel_spindle_front_right, BEHAVIOR=conn_wheel_spindle_front
join,revolute
ori_wheels_front,
**---------------------------------------
*elset,elset=conn_wheels_front
conn_wheel_spindle_front_left, conn_wheel_spindle_front_right
**---------------------------------------
**********
***Center of mass of the Right_LowerSusp
*Node
*Display Body, INSTANCE=Right_LowerSusp-1
**retained nodes of the Right_LowerSusp
*Node
**94464
**94461
**906347
**971497
**94096,
*******
*Nset, nset=right_lowersusp_all, generate
*******
** Right_LowerSusp center of mass
*Element, Type=MASS, ELSET=Right_LowerSusp_center_of_mass
*Mass, ELSET=Right_LowerSusp_center_of_mass
0.0078964778
*Element, Type=ROTARYI, ELSET=Right_LowerSusp_rotary_center_of_mass
*ROTARY INERTIA, ELSET=Right_LowerSusp_rotary_center_of_mass
115.0341, 142.2430, 224.0659
*******
** Right_LowerSusp retained nodes
*Element, Type=MASS, ELSET=Right_LowerSusp_retained_nodes_mass
*MASS, ELSET=Right_LowerSusp_retained_nodes_mass
1.e-5
*Element, Type=ROTARYI, ELSET=Right_LowerSusp_rotary_retained_nodes
*ROTARY INERTIA, ELSET=Right_LowerSusp_rotary_retained_nodes
0.01, 0.01, 0.02
*******
*Element, Type=CONN3D2, ELSET=Right_LowerSusp_db_retained_nodes1
*Connector section, ELSET=Right_LowerSusp_db_retained_nodes1
beam
*Element, Type=CONN3D2, ELSET=Right_LowerSusp_db_retained_nodes
*Connector section, ELSET=Right_LowerSusp_db_retained_nodes, Behavior=sbehavior
cardan, cartesian,
Ori1
**
*********************************************************
**** connector definitions from the tr_conn_brake_right.inp file
*********************************************************
**---------------------------------------
*ELEMENT, TYPE=CONN3D2, ELSET=conn_lower_arm_join_right
*CONNECTOR SECTION, ELSET=conn_lower_arm_join_right
join
**---------------------------------------
*ORIENTATION,NAME=conn_lower_arm_front_right
 0.96942932E+00,   0.24457698E+00,   -0.19720536E-01,    0.24457698E+00,   - 0.96942932E+00,   0.00000000E+00
**********
***Center of mass of the Right_UpperSusp
*Node
*Display Body, INSTANCE=Right_UpperSusp-1
**retained nodes of the Right_UpperSusp
*Node
**903465
**903459
**906345
*******
*Nset, nset=right_uppersusp_all, generate
*******
*Element, Type=MASS, ELSET=Right_UpperSusp_center_of_mass
*Mass, ELSET=Right_UpperSusp_center_of_mass
0.0028383229
*Element, Type=ROTARYI, ELSET=Right_UpperSusp_rotary_center_of_mass
*ROTARY INERTIA, ELSET=Right_UpperSusp_rotary_center_of_mass
20.78962, 38.55819, 45.55291
*******
** Right_UpperSusp retained nodes
*Element, Type=MASS, ELSET=Right_UpperSusp_retained_nodes_mass
*MASS, ELSET=Right_UpperSusp_retained_nodes_mass
1.e-5
*Element, Type=ROTARYI, ELSET=Right_UpperSusp_rotary_retained_nodes
*ROTARY INERTIA, ELSET=Right_UpperSusp_rotary_retained_nodes
0.01, 0.01, 0.02
*******
*Element, Type=CONN3D2, ELSET=Right_UpperSusp_db_retained_nodes
*Connector section, ELSET=Right_UpperSusp_db_retained_nodes, Behavior=sbehavior
cardan, cartesian
Ori1
**---------------------------------------
**********
***Display body for the road
*Node
*Display Body, INSTANCE=Road-1
*Element, Type=MASS, ELSET=road_element
*Mass, ELSET=road_element
0.1
**---------------------------------------
**------------------------------------------------
**------------------------------------------------
**---------------------------------------------------------------
**
**                  BED AND CHASSIS
**
**---------------------------------------------------------------
*ELEMENT, TYPE=CONN3D2, ELSET=conn_bed_chassis
*CONNECTOR SECTION, ELSET=conn_bed_chassis
 join
*ELEMENT, TYPE=CONN3D2, ELSET=conn_bed_chassis1
*CONNECTOR SECTION, ELSET=conn_bed_chassis1
join
**---------------------------------------------------------------
**
**                  FUEL TANK AND CHASSIS
**
**---------------------------------------------------------------
*ELEMENT, TYPE=CONN3D2, ELSET=conn_fuel_tank_chassis
*CONNECTOR SECTION, ELSET=conn_fuel_tank_chassis
join,
**---------------------------------------------------------------
**
**                  BUMPER AND CHASSIS
**
**---------------------------------------------------------------
*ELEMENT, TYPE=CONN3D2, ELSET=conn_bumper_chassis
*CONNECTOR SECTION, ELSET=conn_bumper_chassis
join,
****---------------------------------------------------------------
****
****                  SEAT AND CABIN
****
****---------------------------------------------------------------
*ELEMENT, TYPE=CONN3D2, ELSET=conn_seat_cabin
*CONNECTOR SECTION, ELSET=conn_seat_cabin
join
**---------------------------------------------------------------
**
**                  DOOR HINGES LEFT AND CABIN
**
**---------------------------------------------------------------
*ORIENTATION,NAME=ori_conn_door_left
*ELEMENT, TYPE=CONN3D2, ELSET=conn_door_hinge_left_cabin
** LOW
** UP
*CONNECTOR SECTION, ELSET=conn_door_hinge_left_cabin, BEHAVIOR=conn_door_hinges_beh
join,revolute
ori_conn_door_left,
**---------------------------------------------------------------
**
**                  DOOR LOCK LEFT AND CABIN
**
**---------------------------------------------------------------
*ELEMENT, TYPE=CONN3D2, ELSET=conn_door_lock_left_cabin_cart
*CONNECTOR SECTION, ELSET=conn_door_lock_left_cabin_cart
cartesian,cardan
ori_conn_door_left,
*ELEMENT, TYPE=CONN3D2, ELSET=conn_door_lock_left_cabin
*CONNECTOR SECTION, ELSET=conn_door_lock_left_cabin
axial,
**---------------------------------------------------------------
**
**                  DOOR HINGES RIGHT AND CABIN
**
**---------------------------------------------------------------
*ORIENTATION,NAME=ori_conn_door_right
*ELEMENT, TYPE=CONN3D2, ELSET=conn_door_hinge_right_cabin
** LOW
** UP
*CONNECTOR SECTION, ELSET=conn_door_hinge_right_cabin, BEHAVIOR=conn_door_hinges_beh
join,revolute
ori_conn_door_right,
**---------------------------------------------------------------
**
**                  DOOR LOCK RIGHT AND CABIN
**
**---------------------------------------------------------------
*ELEMENT, TYPE=CONN3D2, ELSET=conn_door_lock_right_cabin_cart
*CONNECTOR SECTION, ELSET=conn_door_lock_right_cabin_cart
cartesian,cardan
ori_conn_door_right,
*ELEMENT, TYPE=CONN3D2, ELSET=conn_door_lock_right_cabin
*CONNECTOR SECTION, ELSET=conn_door_lock_right_cabin
axial,
**---------------------------------------------------------------
**
**                  HOOD HINGES AND CABIN
**
**---------------------------------------------------------------
*ORIENTATION,NAME=ori_conn_hood
*ELEMENT, TYPE=CONN3D2, ELSET=conn_hood_hinges_cabin
** LEFT
** RIGHT
*CONNECTOR SECTION, ELSET=conn_hood_hinges_cabin, BEHAVIOR=conn_hood_hinges_beh
join,revolute
ori_conn_hood,
**---------------------------------------------------------------
**
**                  HOOD LOCK AND CABIN
**
**---------------------------------------------------------------
*ELEMENT, TYPE=CONN3D2, ELSET=conn_hood_lock_cabin_cart
*CONNECTOR SECTION, ELSET=conn_hood_lock_cabin_cart
cartesian,cardan
ori_conn_hood,
*ELEMENT, TYPE=CONN3D2, ELSET=conn_hood_lock_cabin
*CONNECTOR SECTION, ELSET=conn_hood_lock_cabin
axial,
**---------------------------------------------------------------
*elset,elset=conn_all_hood
conn_hood_hinges_cabin,
conn_hood_lock_cabin_cart, conn_hood_lock_cabin
**---------------------------------------------------------------
**---------------------------------------------------------------
**
**                  CABIN AND CHASSIS
**
**---------------------------------------------------------------
*ELEMENT, TYPE=CONN3D2, ELSET=conn_cabin_chassis
*CONNECTOR SECTION, ELSET=conn_cabin_chassis
beam,
*ELEMENT, TYPE=CONN3D2, ELSET=conn_cabin_chassis1
*CONNECTOR SECTION, ELSET=conn_cabin_chassis1, Behavior=sbehavior
cardan, cartesian
Ori1
**---------------------------------------------------------------
**
**                  RADIATOR (CABIN) AND CHASSIS
**
**---------------------------------------------------------------
*ELEMENT, TYPE=CONN3D2, ELSET=conn_radiator_cabin_chassis
*CONNECTOR SECTION, ELSET=conn_radiator_cabin_chassis
beam,
******---------------------------------------
*elset,elset=conn_all_cabin
conn_cabin_chassis,conn_radiator_cabin_chassis,
**conn_yaw_pitch_roll,conn_lateral_acceleration
**---------------------------------------------------------------
**
**                  DRIVESHAFT TO ENGINE
**
**---------------------------------------------------------------
*orientation,name=ori_univ_transm_and_axle
*orientation,name=ori_univ_driveshaft
*element, type=conn3d2, elset=conn_driveshaft_transmission
*connector section, elset=conn_driveshaft_transmission, behavior=driveshaft
join,universal
ori_univ_transm_and_axle, ori_univ_driveshaft
**---------------------------------------------------------------
**
**                  DRIVESHAFT TO REAR AXLE
**
**---------------------------------------------------------------
*element, type=conn3d2, elset=conn_driveshaft_rear_axle
*connector section, elset=conn_driveshaft_rear_axle, behavior=driveshaft
join,universal
ori_univ_driveshaft,ori_univ_transm_and_axle
*elset,elset=conn_driveshaft
conn_driveshaft_transmission, conn_driveshaft_rear_axle
**---------------------------------------
**---------------------------------------
*orientation,name=ori_susp_rear_hinges
**---------------------------------------
**---------------------------------------
**---------------------------------------------------------------
**
**                   LEAF SPRING LEFT
**
**---------------------------------------------------------------
*ELEMENT, TYPE=CONN3D2, ELSET=conn_susp_axle_rear_left
 91000161, 10000003, Leaf_springs-1.821017
*CONNECTOR SECTION, ELSET=conn_susp_axle_rear_left
beam,
**---------------------------------------
*ELEMENT, TYPE=CONN3D2, ELSET=conn_susp_chassisFR_rear_left
 91000162, 20000045, Leaf_springs-1.821022
*CONNECTOR SECTION, ELSET=conn_susp_chassisFR_rear_left,behavior=prevSuspRearHinges
join,revolute
ori_susp_rear_hinges,
**---------------------------------------
*ELEMENT, TYPE=CONN3D2, ELSET=conn_susp_chassisBA_rear_left
 91000163, 20000046, Leaf_springs-1.821023
*CONNECTOR SECTION, ELSET=conn_susp_chassisBA_rear_left,behavior=prevSuspRearHinges
join,revolute
ori_susp_rear_hinges,
**---------------------------------------------------------------
**
**                   LEAF SPRING RIGHT
**
**---------------------------------------------------------------
*ELEMENT, TYPE=CONN3D2, ELSET=conn_susp_axle_rear_right
 91000164, 10000003, Leaf_springs-1.821000
*CONNECTOR SECTION, ELSET=conn_susp_axle_rear_right
beam
**---------------------------------------
*ELEMENT, TYPE=CONN3D2, ELSET=conn_susp_chassisFR_rear_right
 91000165, 20000047, Leaf_springs-1.821005
*CONNECTOR SECTION, ELSET=conn_susp_chassisFR_rear_right,behavior=prevSuspRearHinges
join,revolute
ori_susp_rear_hinges,
**---------------------------------------
*ELEMENT, TYPE=CONN3D2, ELSET=conn_susp_chassisBA_rear_right
 91000166, 20000048, Leaf_springs-1.821006
*CONNECTOR SECTION, ELSET=conn_susp_chassisBA_rear_right,behavior=prevSuspRearHinges
join, revolute
ori_susp_rear_hinges,
**---------------------------------------
*elset,elset=conn_leaf_springs
conn_susp_axle_rear_left,
conn_susp_chassisFR_rear_left, conn_susp_chassisBA_rear_left,
conn_susp_axle_rear_right,
conn_susp_chassisFR_rear_right,conn_susp_chassisBA_rear_right,
**---------------------------------------
*elset,elset=conn_all_leaf_springs
conn_leaf_springs,
**------------------------------------------
**
**                  ENGINE AND CHASSIS
**
**------------------------------------------
*ORIENTATION,NAME=conn_engine_mtg_front_ori
*ELEMENT, TYPE=CONN3D2, ELSET=conn_engine_mtg_front_left_chassis
*CONNECTOR SECTION, ELSET=conn_engine_mtg_front_left_chassis, BEHAVIOR=conn_engine_mtg_front_beh
cartesian,cardan
conn_engine_mtg_front_ori,
**---------------------------------------
*ELEMENT, TYPE=CONN3D2, ELSET=conn_engine_mtg_front_right_chassis
*CONNECTOR SECTION, ELSET=conn_engine_mtg_front_right_chassis, BEHAVIOR=conn_engine_mtg_front_beh
cartesian,cardan
conn_engine_mtg_front_ori,
**---------------------------------------
*ELEMENT, TYPE=CONN3D2, ELSET=conn_engine_mtg_rear_chassis
*CONNECTOR SECTION, ELSET=conn_engine_mtg_rear_chassis, BEHAVIOR=conn_engine_mtg_rear_beh
axial,
**---------------------------------------
*orientation,name=ori_horiz_eng
*ELEMENT, TYPE=CONN3D2, ELSET=conn_engine_mtg_rear_chassis_slide
*CONNECTOR SECTION, ELSET=conn_engine_mtg_rear_chassis_slide
slide-plane,
ori_horiz_eng,
*elset,elset=conn_engine
conn_engine_mtg_front_left_chassis, conn_engine_mtg_front_right_chassis,
conn_engine_mtg_rear_chassis, conn_engine_mtg_rear_chassis_slide
**---------------------------------------------------------------
*elset,elset=conn_all_engine
conn_engine_mtg_front_left_chassis,conn_engine_mtg_front_right_chassis,
conn_engine_mtg_rear_chassis,conn_engine_mtg_rear_chassis_slide
**---------------------------------------
*ELEMENT, TYPE=CONN3D2, ELSET=conn_upper_arm_join_right
*CONNECTOR SECTION, ELSET=conn_upper_arm_join_right
join,
**---------------------------------------
*ORIENTATION,NAME=conn_upper_arm_front_right
**------------------------------------------
**
**                  TIE-RODS, WHEELS,
**                  AND CHASSIS
**
**------------------------------------------
*element,type=conn3d2,elset=conn_steer_left
91000151, LeftTieRod-1.1860663, 20000283
*connector section,elset=conn_steer_left, behavior=beh_tie_rod_prevRigRot_left
join, cardan
Ori1
**
*ORIENTATION,NAME=ori_tie_rod_prevRigRot_left
*element,type=conn3d2,elset=conn_tie_rod_prevRigRot_left
91000152, LeftTieRod-1.172847, RackRod-1.272847
*connector section, elset=conn_tie_rod_prevRigRot_left, behavior=beh_tie_rod_prevRigRot_left
join,cardan
ori_tie_rod_prevRigRot_left,
**---------------------------------------
*element, type=conn3d2, elset=conn_steer_right
91000153, RightTieRod-1.1905294, 20000293
*connector section,elset=conn_steer_right, behavior=beh_tie_rod_prevRigRot_right
join, cardan
Ori1
**
*ORIENTATION, NAME=ori_conn_tie_rod_prevRigRot_right
*element, type=conn3d2, elset=conn_tie_rod_prevRigRot_right
91000154, RightTieRod-1.175462, RackRod-1.275462
*connector section, elset=conn_tie_rod_prevRigRot_right, behavior=beh_tie_rod_prevRigRot_right
join,cardan
ori_conn_tie_rod_prevRigRot_right,
**--------------------------------------
**--------------------------------------
** connection to the left lower A-arm
*ELEMENT, TYPE=CONN3D2, ELSET=conn_stabilizer_left
91000155, Stabilizer-1.207023, 20000305
*CONNECTOR SECTION, ELSET=conn_stabilizer_left
join
**--------------------------------------
** connection to the right lower A-arm
*ELEMENT, TYPE=CONN3D2, ELSET=conn_stabilizer_right
91000156, Stabilizer-1.207000, 20000325
*CONNECTOR SECTION, ELSET=conn_stabilizer_right
join
**--------------------------------------
**--------------------------------------
**--------------------------------------
**
**                 FRONT LEFT AARM HINGES
**
**--------------------------------------
*ORIENTATION,NAME=conn_upper_arm_front_left
*ELEMENT, TYPE=CONN3D2, ELSET=conn_upper_arm_front_left
*CONNECTOR SECTION, ELSET=conn_upper_arm_front_left, BEHAVIOR=conn_arm_hinges_left
join,revolute
conn_upper_arm_front_left,
**-----------------------------------------------
*ORIENTATION,NAME=conn_upper_arm_back_left
*ELEMENT, TYPE=CONN3D2, ELSET=conn_upper_arm_back_left
*CONNECTOR SECTION, ELSET=conn_upper_arm_back_left, BEHAVIOR=conn_arm_hinges_left
join,revolute
conn_upper_arm_back_left,
**--------------------------------------
*ORIENTATION,NAME=conn_lower_arm_front_left
*ELEMENT, TYPE=CONN3D2, ELSET=conn_lower_arm_front_left
*CONNECTOR SECTION, ELSET=conn_lower_arm_front_left, BEHAVIOR=conn_arm_hinges_left
join,revolute
conn_lower_arm_front_left,
**---------------------------------------
*ORIENTATION,NAME=conn_lower_arm_back_left
*ELEMENT, TYPE=CONN3D2, ELSET=conn_lower_arm_back_left
*CONNECTOR SECTION, ELSET=conn_lower_arm_back_left, BEHAVIOR=conn_arm_hinges_left
join,revolute
conn_lower_arm_back_left,
**---------------------------------------
*ELEMENT, TYPE=CONN3D2, ELSET=conn_strut_left
*CONNECTOR SECTION, ELSET=conn_strut_left, BEHAVIOR=conn_strut_left
AXIAL,
**---------------------------------------
*ELEMENT, TYPE=CONN3D2, ELSET=conn_strut_left_stops
*CONNECTOR SECTION, ELSET=conn_strut_left_stops, BEHAVIOR=conn_strut_left_stops
AXIAL,
**---------------------------------------
*elset,elset=conn_all_left_susp
conn_upper_arm_front_left,conn_upper_arm_back_left,
conn_lower_arm_front_left,conn_lower_arm_back_left,
conn_strut_left, conn_strut_left_stops
**
**--------------------------------------
**
**                    FRONT RIGHT AARMS HINGES
**
**--------------------------------------
*ELEMENT, TYPE=CONN3D2, ELSET=conn_upper_arm_front_right
*CONNECTOR SECTION, ELSET=conn_upper_arm_front_right, BEHAVIOR=conn_arm_hinges_right
join,revolute
conn_upper_arm_front_right,
**--------------------------------------
*ORIENTATION,NAME=conn_upper_arm_back_right
*ELEMENT, TYPE=CONN3D2, ELSET=conn_upper_arm_back_right
*CONNECTOR SECTION, ELSET=conn_upper_arm_back_right, BEHAVIOR=conn_arm_hinges_right
join,revolute
conn_upper_arm_back_right,
**--------------------------------------
*ELEMENT, TYPE=CONN3D2, ELSET=conn_lower_arm_front_right
*CONNECTOR SECTION, ELSET=conn_lower_arm_front_right, BEHAVIOR=conn_arm_hinges_right
join,revolute
conn_lower_arm_front_right,
**---------------------------------------
*ORIENTATION,NAME=conn_lower_arm_back_right
*ELEMENT, TYPE=CONN3D2, ELSET=conn_lower_arm_back_right
*CONNECTOR SECTION, ELSET=conn_lower_arm_back_right, BEHAVIOR=conn_arm_hinges_right
join,revolute
conn_lower_arm_back_right,
**---------------------------------------
*ELEMENT, TYPE=CONN3D2, ELSET=conn_strut_right
*CONNECTOR SECTION, ELSET=conn_strut_right, BEHAVIOR=conn_strut_right
AXIAL,
**---------------------------------------
*ELEMENT, TYPE=CONN3D2, ELSET=conn_strut_right_stops
*CONNECTOR SECTION, ELSET=conn_strut_right_stops, BEHAVIOR=conn_strut_right_stops
AXIAL,
**---------------------------------------
*elset,elset=conn_struts
conn_strut_right,conn_strut_right_stops
*elset,elset=conn_all_right_susp
conn_upper_arm_front_right, conn_upper_arm_back_right,
conn_lower_arm_front_right, conn_lower_arm_back_right,
conn_strut_right,conn_strut_right_stops
**
**--------------------------------------
*ORIENTATION,NAME=ori_rack_steering
*ELEMENT, TYPE=CONN3D2, ELSET=conn_rack_steering
91000183, 20000029, RackRod-1.3775462
*CONNECTOR SECTION, ELSET=conn_rack_steering
slot,align
ori_rack_steering,
*nset,nset=rack_and_pinion
**---------------------------------------
*elset,elset=conn_all_steering
conn_steer_left, conn_steer_right, conn_rack_steering
**
**--------------------------------------
**
**                    STABILIZER BAR AND CHASSIS
**
**--------------------------------------
*ORIENTATION,NAME=ori_stab_chassis
*ELEMENT, TYPE=CONN3D2, ELSET=conn_stab_chassis
91000184, 20000027, Stabilizer-1.207008
91000185, 20000028, Stabilizer-1.207015
*CONNECTOR SECTION, ELSET=conn_stab_chassis
slot,
ori_stab_chassis,
**---------------------------------------
****---------------------------------------
****
****                   MEASURING CONNECTORS
****
****-----------------------------------------
*orientation,name=ori_global_cg
*element,type=conn3d2,elset=conn_yaw_pitch_roll
*connector section,elset=conn_yaw_pitch_roll
join, cardan
ori_global_cg,
*nset,nset=accelerometer-cg-shadow
*elset, elset=QA_TEST
conn_yaw_pitch_roll
**---------------------------------------
***element,type=conn3d2,elset=conn_lateral_acceleration
**91000192, 20000220, 39900220
***connector section, elset=conn_lateral_acceleration
**cartesian,
**ori_global_cg,
***nset,nset=accelerometer-cg-ground
**39900220,
**---------------------------------------
**---------------------------------------
*elset,elset=conn_all
conn_cabin_chassis, conn_radiator_cabin_chassis,
**conn_yaw_pitch_roll, conn_lateral_acceleration
**---------------------------------------
*elset, elset=conn_wheels
conn_wheel_spindle_rear_left,conn_wheel_spindle_rear_right
conn_wheel_spindle_front_left,conn_wheel_spindle_front_right
**---------------------------------------
*Elset, elset=everything_all
Stabilizer-1.EVERYTHING_STABILIZER,
LeftTieRod-1.EVERYTHING_LEFT_TIE_RODS
RightTieRod-1.EVERYTHING_RIGHT_TIE_RODS
RackRod-1.EVERYTHING_RACK_RODS
Leaf_springs-1.EVERYTHING_REAR_SUSP_LEAF_SPRINGS
**************************************************************
**    MPCs between the UEL nodes and the nodes on the brakes and rear axle
**************************************************************
*MPC
tie, tire_front_lt_uel-1.50000001, 20000284
tie, tire_front_rt_uel-1.50000002, 20000294
tie, tire_rear_lt_uel-1.50000003, 20000064
tie, tire_rear_rt_uel-1.50000004, 20000065
**------------------------------------------------
*nset,nset=output_red
*nset,nset=all_important_nodes
bed_all, chassis_all, fuel_tank_all, bumper_all,
cabin_all, seat_all, left_door_all, right_door_all,
hood_all, rear_axle_all,
back_lwheel_all, back_rwheel_all,
driveshaft_all, engine_all, front_lwheel_all, brake_left_all,
left_lowersusp_all, left_uppersusp_all, front_rwheel_all,
brake_right_all, right_lowersusp_all, right_uppersusp_all,
Stabilizer-1.BEAM_NODES, Leaf_Springs-1.BEAM_NODES,
RackRod-1.ALL_NODES, LeftTieRod-1.ALL_NODES,
RightTieRod-1.ALL_NODES, tire_front_lt_uel-1.50000001,
tire_front_rt_uel-1.50000002, tire_rear_lt_uel-1.50000003,
tire_rear_rt_uel-1.50000004
*Nset, nset=wheel_spindles
*End Assembly
**--------------------------------------
**--------------------------------------
**--------------------------------------
*********************************************************
**** connector behavior from the tr_conn_door_left.inp file
*********************************************************
*CONNECTOR BEHAVIOR, NAME=conn_door_hinges_beh
*CONNECTOR ELASTICITY,COMPONENT=4
*********************************************************
**** connector behavior from the tr_conn_hood.inp file
*********************************************************
*CONNECTOR BEHAVIOR, NAME=conn_hood_hinges_beh
*CONNECTOR ELASTICITY,COMPONENT=4
*********************************************************
*CONNECTOR BEHAVIOR, NAME=sbehavior
*CONNECTOR ELASTICITY, COMPONENT=1
*CONNECTOR ELASTICITY, COMPONENT=2
*CONNECTOR ELASTICITY, COMPONENT=3
*CONNECTOR ELASTICITY, COMPONENT=4
*CONNECTOR ELASTICITY, COMPONENT=5
*CONNECTOR ELASTICITY, COMPONENT=6
*********************************************************
*CONNECTOR BEHAVIOR, NAME=conn_wheel_spindle_back
*CONNECTOR ELASTICITY, COMPONENT=4
*********************************************************
*connector behavior, name=driveshaft
*connector elasticity,component=4
*********************************************************
*connector behavior, name=prevSuspRearHinges
*connector elasticity,comp=4
*********************************************************
*CONNECTOR BEHAVIOR, NAME=conn_engine_mtg_front_beh
*CONNECTOR ELASTICITY, COMPONENT=1
*CONNECTOR ELASTICITY, COMPONENT=2
*CONNECTOR ELASTICITY, COMPONENT=3
*CONNECTOR ELASTICITY, COMPONENT=4
*CONNECTOR ELASTICITY, COMPONENT=5
*CONNECTOR ELASTICITY, COMPONENT=6
*CONNECTOR DAMPING, COMPONENT=1
*CONNECTOR DAMPING, COMPONENT=2
*CONNECTOR DAMPING, COMPONENT=3
*CONNECTOR DAMPING, COMPONENT=4
*CONNECTOR DAMPING, COMPONENT=5
*CONNECTOR DAMPING, COMPONENT=6
***---------------------------------------
*CONNECTOR BEHAVIOR, NAME=conn_engine_mtg_rear_beh
*CONNECTOR ELASTICITY, COMPONENT=1
*CONNECTOR DAMPING, COMPONENT=1
*********************************************************
*CONNECTOR BEHAVIOR, NAME=conn_wheel_spindle_front
*CONNECTOR ELASTICITY, COMPONENT=4
*************************************************
*connector behavior, name=beh_tie_rod_prevRigRot_left
*connector elasticity,comp=4
*connector elasticity,comp=5
*connector elasticity,comp=6
*connector behavior, name=beh_tie_rod_prevRigRot_right
*connector elasticity,comp=4
*connector elasticity,comp=5
*connector elasticity,comp=6
*connector behavior, name=temp
*connector elasticity,comp=4
*connector elasticity,comp=5
*connector elasticity,comp=6
*********************************************************
**** connector behavior from the tr_conn_aarms_left.inp file
*********************************************************
**---------------------------------------
*CONNECTOR BEHAVIOR, NAME=conn_arm_hinges_left
*CONNECTOR ELASTICITY, COMPONENT=4
<conelPrevAarms>,
*connector friction,predefined
*friction
0.0,
**------------------------------------------------
*CONNECTOR BEHAVIOR, NAME=conn_strut_left
*CONNECTOR ELASTICITY, COMPONENT=1
<conelasstrut>,
*CONNECTOR DAMPING, COMPONENT=1
<condampstrut>,
*connector constitutive
<conrefleft>,
**------------------------------------------------
*CONNECTOR BEHAVIOR, NAME=conn_strut_left_stops
*CONNECTOR ELASTICITY, COMPONENT=1, nonlinear
<strut_upper_stop_range_force>,<strut_upper_stop_range>
-0.1,<strut_upper_stop>
 0.1,<strut_lower_stop>
<strut_lower_stop_range_force>,<strut_lower_stop_range>
**---------------------------------------
*CONNECTOR BEHAVIOR, NAME=conn_arm_hinges_right
*CONNECTOR ELASTICITY, COMPONENT=4
<conelPrevAarms>,
*connector friction,predefined
*friction
0.0,
**------------------------------------------------
*CONNECTOR BEHAVIOR, NAME=conn_strut_right
*CONNECTOR ELASTICITY, COMPONENT=1
<conelasstrut>,
*CONNECTOR DAMPING, COMPONENT=1
<condampstrut>,
*connector constitutive
<conrefright>,
**------------------------------------------------
*CONNECTOR BEHAVIOR, NAME=conn_strut_right_stops
*CONNECTOR ELASTICITY, COMPONENT=1,nonlinear
<strut_upper_stop_range_force>,<strut_upper_stop_range>
-0.1, <strut_upper_stop>
 0.1, <strut_lower_stop>
<strut_lower_stop_range_force>,<strut_lower_stop_range>
**---------------------------------------------------------------
*AMPLITUDE,NAME=zero
0,0,1,0
*AMPLITUDE,NAME=ramp
0,0,1,1
*AMPLITUDE,NAME=step
0,1,1,1
*amplitude, name=rampvel, definition=smooth step
0, <init_vel>, <time_accel>, <cruise_velocity>
*amplitude, name=maintainvel
0, <init_vel>, 1, <init_vel>
*amplitude, name=steer-right
0, 0, <time_const_vel_bb_free_step>, 0, <time_steer_right>, <rack_steer_right_max>
*amplitude,definition=periodic,name=sinusoidal_steering
1, <omega>, <time_const_vel_bb_free_step>, 0.0
0.0, <steering_amplitude>
*amplitude,name=spinwheels
0, 0, <total_analysis_time>, <total_spin>
*amplitude,name=steer-steps
0, 0, 0.30, 0.06, 0.75, -0.06, 1.0, 0.0
*amplitude,name=smooth,definition=smooth
0, 0, 1.0, 1.0
**------------------------------------------------
** Initial conditions in the springs of type stress.
**------------------------------------------------
*Include, input=tr_initial_stress_db.inp
**------------------------------------------------
***Initial conditions,type=stress,unbalanced stress=step
**Leaf_springs-1.54771, 2431., -1906., -1037., 1.6885E+06, -8.1282E+05,  1.4602E+05
**Leaf_springs-1.54772, 2193., -2243., -861.1, 1.3174E+06, -6.6449E+05, -9.6597E+04
**Leaf_springs-1.54773, 2105., -2334., -819.5, 9.0551E+05, -5.1820E+05, -1.5653E+05
**Leaf_springs-1.54774, 2201., -2220., -860.0, 5.1063E+05, -3.7148E+05, -1.1478E+05
**Leaf_springs-1.54775, 2494., -1856., -901.6, 1.5658E+05, -2.2535E+05, -5.9346E+04
**Leaf_springs-1.54776, 2479., 1479.,  877.2, 1.2840E+05, -1.2202E+05,  1.3535E+05
**Leaf_springs-1.54777, 1637., 2328., 1014., 4.8665E+05, -2.3177E+05,  1.8984E+05
**Leaf_springs-1.54778, 1342., 2515., 1015., 9.3475E+05, -3.9460E+05,  2.2643E+05
**Leaf_springs-1.54779, 1623., 2349., 1014., 1.3844E+06, -6.0580E+05,  1.6798E+05
**Leaf_springs-1.54780, 2417., 1530., 1011., 1.7399E+06, -8.0521E+05, -1.1715E+05
**Leaf_springs-1.54783, 2996., -2104., -986.7, -1.8918E+06,  7.8522E+05, -1.0822E+05
**Leaf_springs-1.54784, 2714., -2526., -766.6, -1.4748E+06,  6.4478E+05,  1.4611E+05
**Leaf_springs-1.54785, 2608., -2644., -713.3, -1.0093E+06,  5.1463E+05,  2.0898E+05
**Leaf_springs-1.54786, 2722., -2503., -765.5, -5.6352E+05,  3.8763E+05,  1.6476E+05
**Leaf_springs-1.54787, 3055., -2054., -819.6, -1.6861E+05,  2.6409E+05,  1.0420E+05
**Leaf_springs-1.54788, 3076., 1562., 864.1, -1.3856E+05,  9.5933E+04, -8.6937E+04
**Leaf_springs-1.54789, 2153., 2640., 1035., -5.3038E+05,  2.2803E+05, -1.3372E+05
**Leaf_springs-1.54790, 1817., 2885., 1036., -1.0415E+06,  4.0138E+05, -1.7042E+05
**Leaf_springs-1.54791, 2138., 2661., 1035., -1.5543E+06,  6.0981E+05, -1.1144E+05
**Leaf_springs-1.54792, 3014., 1613., 1031., -1.9464E+06,  7.9063E+05,  1.7094E+05
**------------------------------------------------
**------------------------------------------------
***constraint controls, no checks
*initial conditions, type=velocity
all_important_nodes, 1, <init_vel>
all_important_nodes, 2, 0.0
**------------------------------------------------
**------------------------------------------------
*surface interaction, name=mu
*friction
0.0,
**--------------------------------------
**--------------------------------------
**--------------------------------------
***************************************************
***Step defintions
***************************************************
*step,NLGEOM,inc=1000
*STATIC, direct=nostop
<time_inc_grav>,<total_time_grav>,<time_inc_grav>,<time_inc_grav>
**-------------------------------------------------
*CONTROLS,ANALYSIS=DISCONT
*Boundary
10000023, 1,6
*Boundary
**accelerometer-cg-ground,1,3
accelerometer-cg-shadow,4,6
*Boundary,amplitude=<load_style_grav>
retained_cabin_cg,                    1,2,0
retained_cabin_cg,                    6,6,0
**wheel_spindles,                     3,3,0
**------------
*CONNECTOR MOTION,amplitude=<rack_amplitude>
conn_rack_steering,            1,0.0
**--------------------------------------
***Connector motion from tr_lock_doors_and_hood.inp
**--------------------------------------
*Include, input=tr_lock_doors_and_hood_db.inp
**--------------------------------------
***************************************************
*CONNECTOR MOTION
conn_wheels, 4, 0.0
**------------
*DLOAD,amplitude=<load_style_grav>
everything_all,GRAV,<grav_acceler>,0,0,-1
**--------------------------------------------------
*OUTPUT,FIELD, var=preselect
*element output
s
*node output
u, CF
*node output
u,
*output,history
*node output,nset=wheel_spindles
u1, u2, u3
*node output,nset=wheel_spindles
u,v
*Element Output, elset=conn_yaw_pitch_roll
CU
*node print,nset=wheel_spindles,summary=no
u,
*END STEP
**------------------------------------------------
**------------------------------------------------
**
** Get vehicle up to speed
**
*step,nlgeom,inc=1000000
*dynamic,direct,alpha=-0.05,initial=yes,nohaf, singular mass=warning
<time_inc_accel>,<total_time_accel_step>
**--------------
*CONTROLS,ANALYSIS=DISCONT
*boundary,amp=rampvel,type=velocity,op=new
10000002, 1,1,1.0
**-------------
*boundary,op=new
accelerometer-cg-shadow,4,6
*CONNECTOR MOTION,amplitude=<rack_amplitude>
conn_rack_steering, 1, 0.0
*CONNECTOR MOTION
conn_wheels,4,0.0
**--------------
*OUTPUT,FIELD, var=preselect, frequency=5
*node output
u, CF
*node output
u,
*output,history, frequency=5
*node output, nset=retained_chassis
u, v
*node output,nset=wheel_spindles
u,v
*Element Output, elset=conn_yaw_pitch_roll
CU
*end step
**------------------------------------------------
**------------------------------------------------
**------------------------------------------------
**
** Truck over the bump OR steering
**
*STEP, NLGEOM,INC=10000000
*DYNAMIC, alpha=-0.05, INITIAL=yes, haftol=1.e6, singular mass=warning
<time_inc_cruise>,<total_analysis_time>,<time_inc_cruise_min>,<time_inc_cruise_max>
*elset, elset=connfrics
conn_upper_arm_front_left,conn_upper_arm_back_left,
conn_lower_arm_front_left,conn_lower_arm_back_left,
conn_upper_arm_front_right,conn_upper_arm_back_right,
conn_lower_arm_front_right,conn_lower_arm_back_right,
*change friction, elset=connfrics
*friction
0.12,
**
**         rack-pinion motion
**
*CONNECTOR MOTION, amplitude=<rack_amplitude>
conn_rack_steering, 1, 0.0
**
****
****        Spin the wheels
****
*CONNECTOR MOTION, amplitude=spinwheels
conn_wheels,4,0.0
**--------------
*OUTPUT, FIELD
*node output
u,
*output, history
*node output,nset=wheel_spindles
u,v
*Element Output, elset=conn_yaw_pitch_roll
CU
*Element Output, elset=QA_TEST
CUR2, CUR3
**--------------
*END STEP
**------------------------------------------------