*Node
*Nset, Nset=LeftNode
*nset, nset=qa_test_leftnode
*Nset, Nset=RightNode
*nset, nset=qa_test_rightnode
*orientation, name=oria
*elset,elset=qa_test_AllElements
*Element, Type=CONN3D2, Elset=AllElements
*Connector section, Elset=AllElements, behavior=elas
SLOT,
oria,
*connector behavior, name=elas
*connector elasticity, comp=1
*element, type=mass,elset=mass
*mass,elset=mass
0.1
*Amplitude, Name=LoadAmp
0,0,1,1
**------------------------------------------------
*Node
*Nset, Nset=LeftNode2
*nset, nset=qa_test_leftnode2
*Nset, Nset=RightNode2
*nset, nset=qa_test_rightnode2
*elset,elset=qa_test_AllElements2
*Element, Type=CONN3D2, Elset=AllElements2
*Connector section, Elset=AllElements2, behavior=elas
SLOT,
oria,
*element, type=mass,elset=mass2
*mass,elset=mass2
0.1
*Amplitude, Name=LoadAmp2, Definition=User, Variables=1
**------------------------------------------------
*filter, type=butterworth, name=sae60
**------------------------------------------------
*Step,Nlgeom=Yes
*Dynamic, Explicit,direct
 0.001, 1.0
*Variable Mass Scaling, type=below min, Dt=1.0e-3, freq=2
**-----------
**
*CLOAD
 RightNode , 2, 1.0
 RightNode2, 2, 1.0
*Boundary, , Amplitude=LoadAmp
 LeftNode, 1, 1, -1.0
 LeftNode, 2, 6, 0.0
 LeftNode2, 1, 1, -1.0
 LeftNode2, 2, 6, 0.0
*BOUNDARY, Amplitude=LoadAmp
 RightNode, 1, 1, 1.0
*BOUNDARY, Amplitude=LoadAmp2
 RightNode2, 1, 1, 1.0
*Output, Field, Var=preselect
**------
*OUTPUT,HISTORY,TIME INT=1.e-2, SENSOR, name=RightNodeSensor_U1
*NODE OUTPUT, NSET=RightNode
u1,
*OUTPUT,HISTORY,freq=1, SENSOR, name=LeftNodeSensor_U1, FILTER=sae60
*NODE OUTPUT, NSET=LeftNode
u1,
*OUTPUT,HISTORY,freq=1, SENSOR, name=LeftNodeSensor2_U1
*NODE OUTPUT, NSET=LeftNode2
u1,
*OUTPUT,HISTORY,TIME INT=1.e-2, SENSOR, name=ELEM1_SENSOR_CU1
*ELEMENT OUTPUT, ELSET=AllElements
CU1,
*Output,History,freq=1, Sensor, Name=Elem1_Sensor_Crf2, FILTER=sae60
*Element Output, Elset=Allelements
Ctf2,
*Output,History,freq=1, Sensor, Name=Elem2_Sensor_CU1
*Element Output, Elset=Allelements2
CU1,
**------
*Output, History, Freq=1
*Node Output, Nset=LeftNode
 U1, RF1
*Node Output, Nset=LeftNode2
 U1, RF1
*Node Output, Nset=RightNode
 U1, RF1
*Node Output, Nset=RightNode2
 U1, RF1
*element output, elset=qa_test_AllElements
CEF1,
*element output, elset=qa_test_AllElements2
CEF1,
*Energy Output
*End Step
**------------------------------------------------
*Step,Nlgeom=Yes
*Dynamic, Explicit,direct
 0.001 , 1.0
*Variable Mass Scaling, type=below min, Dt=1.0e-3, freq=2
*CLOAD
 RightNode , 2, 1.0
 RightNode2, 2, 1.0
*Boundary, , Amplitude=LoadAmp
 LeftNode, 1, 1, -1.0
 LeftNode, 2, 6, 0.0
 LeftNode2, 1, 1, -1.0
 LeftNode2, 2, 6, 0.0
*BOUNDARY, Amplitude=LoadAmp
 RightNode, 1, 1, 1.0
*BOUNDARY, Amplitude=LoadAmp2
 RightNode2, 1, 1, 1.0
*Output, Field, Var=preselect
*OUTPUT,HISTORY,TIME INT=1.e-2, SENSOR, name=RightNodeSensor_U1
*NODE OUTPUT, NSET=RightNode
u1,
*OUTPUT,HISTORY,TIME INT=1.e-2
*ELEMENT OUTPUT, ELSET=AllElements
CU1,
*Output,History,freq=1, FILTER=sae60
*Element Output, Elset=Allelements
Ctf2,
*Element Output, Elset=Allelements2
Ctf2,
*Node Output, Nset=LeftNode
 U1, RF1
*Node Output, Nset=LeftNode2
 U1, RF1
*Node Output, Nset=RightNode
 U1, RF1
*Node Output, Nset=RightNode2
 U1, RF1
*End Step
**------------------------------------------------