*HEADING
 Transfer from Explicit to Standard : Plasticity Test for CAX3 element
 - Standard Analysis
 - Plastic material with combined hardening (multiple backstresses)
*IMPORT,STEP=1,INT=2,UPDATE=NO,STATE=YES
 SHELL,
*IMPORT NSET
 ALL,
*BOUNDARY
 1, 1,2
 2, 2,2
 4, 1,1
*RESTART, WRITE, FREQ=100
**
**
*NSET, NSET=QA_TEST_ALLNODES
ALL,
**
*STEP,NLGEOM,INC=50
*STATIC
 0.1, 1.
*BOUNDARY
3,1,1,0.016
2,1,1,0.016
*PRINT,FREQ=1
*EL PRINT
 PEEQ,
 MISES,
 ALPHA
*NODE PRINT
 U,
 COORD,
 RF,
*OUTPUT,FIELD,VARIABLE=PRESELECT,FREQUENCY=100
*OUTPUT,FIELD
*ELEMENT OUTPUT
 S,PEEQ,ALPHA,ALPHAN
*NODE OUTPUT
 U,COORD
*OUTPUT,HISTORY
*NODE OUTPUT, NSET=QA_TEST_ALLNODES
 U,COORD
*END STEP