*HEADING
 Transfer from Standard to Explicit : MPC tie
 - Standard analysis
 [base for sx_x_cps4r_mpctie, references xs_x_cps4r_mpctie]
*IMPORT,UPDATE=NO,STATE=YES
ELALL,
*RESTART,WRITE
*MPC
TIE, 2,5
TIE, 3,8
**
** STEP #1
**
**
*STEP,NLGEOM
*STATIC
0.1,1.0
*BOUNDARY
LEFT,  1,1,
BOTTOM,2,2,
RIGHT, 1,1, 0.2
*NODE PRINT
U,
*EL PRINT, ELSET=ELALL
S,
*OUTPUT,FIELD,VARIABLE=PRESELECT,FREQUENCY=9999
*OUTPUT,FIELD
*NODE OUTPUT
U,
*OUTPUT,HISTORY
*NODE OUTPUT, NSET=QA_TEST_ALLNODES
U,
*OUTPUT,FIELD
*ELEMENT OUTPUT,ELSET=ELALL
S,
*OUTPUT,HISTORY
*ELEMENT OUTPUT,ELSET=ELALL
S,
*END STEP