*HEADING
 Transfer from Explicit to Standard : Test for S4RT element
*IMPORT,UPDATE=NO,STATE=YES
 EALL,
*IMPORT NSET
 LEFT,BOT,TOP
*NSET,NSET=all
*BOUNDARY
 LEFT,1,6
 BOT,2,6
 BOT,11,15
 TOP,4,6
** 1, 1,2
** 2, 1,2
** 3, 2,2
** 4, 2,2
*RESTART, WRITE, FREQ=100
**
*STEP,NLGEOM,INC=50
*COUPLED TEMPERATURE-DISPLACEMENT, STEADY STATE
 0.1, 1.
**BOUNDARY
**3,11,,0.
**CONTROLS, PARAMETERS=FIELD, FIELD=DISPLACEMENT
** 5.e-4,,,,
*OUTPUT,HISTORY,FREQUENCY=1
*ENERGY OUTPUT,VARIABLE=PRESELECT
*OUTPUT,FIELD
*NODE OUTPUT
RF,
NT,
RFL,
U,
COORD,
*ELEMENT OUTPUT
 S,FV,TEMP
*END STEP