HEADING
 Transfer from Explicit to Explicit : Test for all acoustic elements
*IMPORT, UPDATE=NO, STATE=YES, STEP=1
A2D,A3D,AAXI
*IMPORT NSET
QA_TEST_All_NSETS_AUTO,BOTTOM,TOP
*BOUNDARY
BOTTOM,8,8
*RESTART, WRITE
**
*STEP
*DYNAMIC, EXPLICIT
, 1.E-3
*BOUNDARY
TOP,8,8,1.
*OUTPUT,FIELD,VARIABLE=PRESELECT,NUMBER INTERVAL=4,OP=NEW
*OUTPUT,HISTORY,VARIABLE=PRESELECT,TIME INTERVAL=0.0025,OP=NEW
*OUTPUT, FIELD,TIMEMARKS=YES,NUM=1
*NODE OUTPUT,NSET=QA_TEST_All_NSETS_AUTO
 POR,
*END STEP