*HEADING
 Transfer from Explicit to Explicit : Test for all elements with
 inelastic material
*IMPORT, UPDATE=NO, STATE=NO, STEP=1
T2D2PLAS,T3D2PLAS,B21PLAS,B22PLAS,B31PLAS,B32PLAS
SHELLPLAS,SHELLHILL,SHELLCRACK,SHELLDAMP,SHELLGLASS_EPOXY
CPSPLAS,CPSCRACK,CPSDAMP,CPSGLASS_EPOXY
CPEPLAS,CPEEOS,CPECRACK,CPEDAMP
CAXPLAS,CAXEOS,CAXCRACK,CAXDAMP
SOLIDPLAS,SOLIDEOS,SOLIDCRACK,SOLIDDAMP
MEMBPLAS,MEMBHILL,MEMBCRACK,MEMBDAMP,MEMBGLASS_EPOXY
SAX1PLAS,SAX1HILL,SAX1CRACK,SAX1GLASS_EPOXY
*IMPORT ELSET
QA_TEST_All_ELSETS_AUTO
**
*BOUNDARY
BOTTOM,2,2
EL3D,3,3
*RESTART, WRITE
**
*STEP
*DYNAMIC, EXPLICIT
, 1.E-3
*BOUNDARY, TYPE=VELOCITY
 TOP, 2, 2, 1.0
*OUTPUT,FIELD,VARIABLE=PRESELECT,NUMBER INTERVAL=4,OP=NEW
*OUTPUT,HISTORY,VARIABLE=PRESELECT,TIME INTERVAL=0.0025,OP=NEW
*OUTPUT, FIELD,TIMEMARKS=YES,NUM=1
*ELEMENT OUTPUT,ELSET=QA_TEST_All_ELSETS_AUTO
 MISESMAX,
 LE,
 TEMP,
 DAMAGEC,
 DAMAGET,
 SDEG,
 CFAILURE,
 DMICRT,
 VS,
 PS,
 PEEQ,
 PEEQT,
*END STEP