*HEADING
 Transfer from Explicit to Explicit : Test for all
 temperature-disp. elements
*IMPORT, UPDATE=YES, STATE=YES, STEP=1
SHELLELAS,SHELLEC,SHELLORTHO,SHELLANISO
CPSELAS,CPSEC,CPSORTHO,CPSANISO,CPSLAMINA
CPEELAS,CPEEC,CPEORTHO,CPEANISO
CAXELAS,CAXEC,CAXORTHO,CAXANISO
SOLIDELAS,SOLIDEC,SOLIDORTHO,SOLIDANISO
*IMPORT ELSET
QA_TEST_All_ELSETS_AUTO
*IMPORT NSET
QA_TEST_All_NSETS_AUTO,EL3D,BOTTOM,TOP
**
*BOUNDARY
BOTTOM,1,2
EL3D,3,3
BOTTOM,11,11,0.0
*RESTART, WRITE
**
*STEP
*DYNAMIC TEMPERATURE-DISPLACEMENT, EXPLICIT
*BOUNDARY, TYPE=VELOCITY
 TOP, 2, 2, 1.0
*BOUNDARY
 TOP, 11,11,100.0
*OUTPUT,FIELD,VARIABLE=PRESELECT,NUMBER INTERVAL=4,OP=NEW
*OUTPUT,HISTORY,VARIABLE=PRESELECT,TIME INTERVAL=0.0025,OP=NEW
*OUTPUT, FIELD,TIMEMARKS=YES,NUM=1
*ELEMENT OUTPUT,ELSET=QA_TEST_All_ELSETS_AUTO
 MISESMAX,
 LE,
 TEMP,
*NODE OUTPUT,NSET=QA_TEST_All_NSETS_AUTO
 U,
 V,
*END STEP